DIVISION 27 21 29
Vi2304A 4-Port MaxiiCopper™ High Speed Ethernet Extenders over UTP Cables
PART 1 – GENERAL
1.01	SUMMARY
A.	Ethernet Extender over UTP Cable

1.02	SECTION INCLUDES
A.	Vi2304A 4-Port Ethernet extender over UTP using Symmetric Bandwidth (SBWTM) and Pass Through PoE (PTPTM) technology. 

1.03	REFERENCES
A.	CE - European Union Compliance (CE)
B.	RoHS - Restriction of Use of Hazardous Substances
C.	WEEE - Waste Electrical and Electronic Equipment Directive
D.	UL, cUL - Underwriters Laboratory
E.	RFC - Request for Comments
F.	IEEE - Institute of Electrical and Electronics Engineers
G.	EN/IEC - International Electrotechnical Commission

1.04	SYSTEM DESCRIPTION
A.	Connection Requirements: Provide Extended Ethernet ports with RJ45 connector and standard 10/100Base-TX RJ45 connector.
1.	The system shall utilize a 1-pair or 4-pair Category 5/5e/6 cables terminated in RJ45 connector with EIA568-B configuration for extended 10Base-T or 100Base-T.
2.	The system shall utilize a 4-pair Category 5/5e/6 cable terminated in RJ45 connector with EIA568-B configuration for standard 10Base-T or 100Base-T.

1.05	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed installation and operating information
B.	Warranty: Manufacturer’s Printed Warranty

1.06	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate controlled environment. 
B.	Storage Temperature not to exceed: -40˚C to +85˚C.

1.07	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of -40˚C to +75˚C without the assistance of fan-forced cooling.
B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 90% (non-condensing). 

1.08	WARRANTY

A.	Limited Life Time Warranty: Vigitron guarantees product to be free of defects for product lifetime, defined as the time that product is in production plus 3 years from end of production.

PART 2 – PRODUCTS
2.01	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc. 7810 Trade Street, Suite 100, San Diego, CA 92121, USA 
2.	Phone 1-858-484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted

2.02	MANUFACTURED UNITS
A.	Reference Table A: Product Number, Descriptions and Maximum Distance
B.	Reference Table B: IEEE Product Compatibility Chart
C.	Reference Table C: Product System Compatibility Chart

2.03	GENERAL SPECIFICATIONS
A.	The 4-port UTP Ethernet extender shall be Vi2304A. 
B.	Standard Ethernet Ports:
1.	The device shall have 8 or 16 10/100BaseT standard Ethernet ports in a compact housing:
a.	The Ethernet port will comply with: 
i.	IEEE 802.3u 10baseT 
ii.	IEEE 802.3u 100baseT 
2.	The Extended and Standard Ports will be compliant to IEC 60603-7.
3.	The device shall support Standard Ethernet UTP connection distances up to 100 meters.
4.	The device will be compliant to 802.3af and 802.3at Type 1 and 2 standards and 60W PoE.
5.	The device will have no switch settings.
6.	The following settings will be done by automatic detection:
a.	Bandwidth
b.	Master/Slave
c.	1-pair or 4-pair UTP
7.	The device shall be used as either master or slave in the same system.
C.	The Extended Distance Ethernet Ports:
1.	Will support distances up to 3,000 feet (914m) at 10BaseT. 
2.	Will support distances up to 2,100 feet (640m) at 100BaseT. 
3.	Will support 10/100BaseT and PoE at following distances:
a.	802.3af at 2,000 feet (609m)
b.	802.3at at 800 feet (243m)
c.	PoE ++ (50W at camera PD) at 500 feet (152m) when used with a 60W PoE source. 
d.	PoE++ (50W at camera PD) at 750 feet (228m) when used with Vi2701RX or Vigitron 74W PoE source (Vi2208A/Vi2216A/Vi2508/Vi2516)
e.	IEEE 802.3af,at,bt PoE compliant to 74W
8.	Will support the ability to pass 802.3af/at and 60W PoE++ from a source to a device at the stated distances to power a PD device.
9.	Will maintain all 802.3af/at safety standards for PSE and PD communications.
10.	Will carry signals at extended distances.
F.	The system will provide the ability to test and verify connection status, and operating bandwidth between two transceivers over the extended connection.
G.	The device will be power by a 12VDC external power supply. 
H.	The device will consume less than 6 W
I.	Devices may serve as either slave or master.
J.	The device shall provide below LED indicators for monitoring proper system operation:
1.	Power - Red indicates power on.
2.	Extended distance traffic/Link – Orange
a.	Off - No traffic
b.	Flashing – Traffic
3.	Extended Bandwidth indication:
a.	10BaseT - Green indicating 10BaseT
b.	100BaseT - Orange indicating 100BaseT
4.	Standard Ethernet Connections: Green
a.	Off indicating no connection 
b.	Flashing - connection with traffic
5.	Standard Ethernet Bandwidth indication
a.	10/100BaseT Yellow
b.	Off - no connection 
c.	On - connection is valid
K.	The device will be compatible with 60W and higher power PoE sources used with Sony and Axis cameras.

2.04	DATA SPECIFICATIONS
A.	Data Interface: Passage of data compliant to: 
1.	RFC 768 UDP
2.	RFC 2068 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 1783 TFTP
6.	RFC 894 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Data Rate: 10/100 Mbps
C.	Data Connections: 
1.	Vi2304A 4 standard Ethernet ports and 4 extended Ethernet ports

2.05	SPECIFICATIONS and FEATURE SETS
A.	The extender device will transmit and receive data using Symmetric Bandwidth (SBW™). 
1.	Bandwidth will be constant over the quoted extended distance with no more than a 5% decrease, when the input signal varies from a size of 64 bytes to 4,500 bytes using bidirectional transmission.
2.	Bandwidth will be constant over the quoted extended distance with no more than 5% decrease when: 
a.	Bidirectional signals are transmitted with a packet size of 4,500 bytes.
b.	Unidirectional signals are transmitted with a packet size of 9,000 bytes.
c.	Bandwidth will remain the same for both upload and download operation.
B.	Packet losses will be at 2% or less at packet sizes, ranging from 64 bytes to 4500 bytes bidirectional and 9,000 bytes unidirectional.
C.	Packet losses will be at 2% or less at packet sizes of 4,500 in bidirectional transmission.
D.	Packets per second (PPS) will not vary more than 5% at packet sizes, ranging from 64 bytes to 4,500 bytes.
E.	Packet per second (PPS) will not vary more than 5% at packet of 4500 bytes in bidirectional transmission.
F.	Maximum distance will be 3,000 feet (914m) at 10BaseT. 
G.	Maximum distance will be 2,100 feet (640m) at 100BaseT. 
H.	Extender device must have the ability to function as Transceiver. 
I.	Extender device must have the ability to be powered using IEEE 802.3at or IEEE 802.3af PoE. 
J.	Extender device must have the ability to operate using Pass Through PoE (PTP™) with a single PoE source, providing power to both transceivers and PD device conforming to 802.3af/at standards. 
K.	Extender device must have the ability to pass through PoE functionality in compliance with IEEE 802.3af/at standards when communicating with a PD: 
1.	Pass through detection pulses from PSE to PD.
2.	Pass through classification pulses from PSE to PD.
3.	Pass through required power from PSE to PD. 
4.	Ability to provide Class 2 802.3af at maximum extended distance to both transceivers and PD from a PoE source. 
5.	Ability to provide Class 0, 1, 2, 3 and 4 802.3af/at power to both transceivers and PD from a PoE source depending on cable length.
L.	Extender must be able to operate in extended temperature environments of -40˚C to +75˚C type tested in compliance to NEMA-TS2 testing procedures.
M.	Extender must provide the ability to test extended distance connection continuity and bandwidth by means of LED indicators. 

2.06	CONNECTORS
A.	Power: IEC 320-C14 inlet
B.	Extended Ethernet RJ45 Port: IEC 60603-7
C.	Standard Ethernet RJ45 Port: IEC 60603-7

2.07	ELECTRICAL SPECIFICATIONS
1.	Power Supply: 	12VDC @ 500mA

2.08	MECHANICAL SPECIFICATIONS
A.	Dimensions (H x W x L): 1.15” x 3.6” x 3.3”, 4.2cm x 9.2cm x 8.4cm
B.	Finish: Device shall be constructed of a metal enclosure. 
C.	Weight: 0.584lb (265g)
D.	Mounting: Shall be able to be wall-mounted. 

2.09	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temperature: -40˚C to +75˚C
B.	Storage Temperature: -40˚C to +85˚C
C.	Relative Humidity: 0% to 90% (non-condensing)

2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS
A.	FCC Part 15, Subpart B, Class B 2010
B.	Emission Standards: 
1.	FCC Part 15, Subpart B, Class B 2010
2.	EN 55022:206+A1:2007
3.	EN61000-3-2:2006+A1:2009+A2:2009
4.	EN 61000-3-3:2008
5.	EN55024:1998+A1:2001+A2:2003
C.	Safety:
1.	CSA C22.2 NO. 60950-1-07-CAN/CSA INFORMATION TECHNOLOGY EQUIPMENT SAFETY PART GENERAL REQUIREMENTS - Edition 2 - Revision Date 2011/12/19
2.	UL 60950-1 INFORMATION TECHNOLOGY EQUIPMENT - SAFETY - PART 1: GENERAL REQUIREMENTS - Edition 2 - Revision Date 2011/12/19
D.	RoHS
E.	CE

2.11	ACCESSORIES
A.	Operation Manual 
B.	Rack mounting brackets

2.12	MANUFACTURED UNITS REFERENCE TABLES

PRODUCT	DESCRIPTION	MAX. DISTANCE*	
Vi2304A  
	Extended Ethernet over UTP	3,000 Feet (914m) @ 10BaseT
2,100 Feet (640m) @ 100BaseT	
Table A: Product Number Descriptions
*Distance and performance figures are obtained using in-house testing mirroring typical installations. Factors such as cabling, connections, use of power and environmental conditions may affect actual distance, and should be taken in consideration.

PRODUCT		COMPATIBLE IEEE STANDARDS	
Vi2304A  
	IEEE 802.3u     IEEE 802.3af      
IEEE 802.3at  
IEEE 802.3at 	Fast Ethernet standard for 10/100TX
Power over Ethernet
Power over Ethernet
Power over Ethernet (up to 74W)	
Table B: Product IEEE Compatibility Chart 

PRODUCT	COMPATIBLE ETHERNET EQUIPMENT	
Vi2304A
	Vi2300A  1-port UTP Ethernet Extender 
Vi2300PW  1-port UTP Ethernet Extender 
Vi2301A  1-port UTP Ethernet Extender
Vi2301A  1-port UTP Ethernet Extender 
Vi2301AU  1-port UTP Ethernet Extender  
Vi2304A  4-port UTP Ethernet Extender
Vi2308A  8-port UTP Ethernet Extender 
Vi2316A  16-port UTP Ethernet Extender 
Vi2804A  4-port Extended PoE Switch
Vi2804AP 4-port Extended PoE Switch 
Vi2208A / Vi2208AS  8-port Midspan
Vi2216A / Vi2216AS  16-port Midspan
Vi2508 / Vi2508S  8-port Extended Midspan 
Vi2516 / Vi2516S  16-port Extended Midspan
Vi2701Rx  1-port UTP Ethernet Extender	
Table C: Product System Compatibility Chart

Vigitron reserves the right to change products or specifications without notice.

END OF SECTION