Author: mngo
Last saved by: ali
Company: Hewlett-Packard Company

DIVISION 27 21 29
Vi2401A MaxiiCopper™ High Speed Ethernet Extenders over Coax Cables
PART 1 - GENERAL
1.01	SUMMARY
A.	Ethernet extender over coax cables

1.02	SECTION INCLUDES
A.	Vi2401A single Port Ethernet extender over Coax using Symmetric Bandwidth (SBW^TM) and Pass Through PoE (PTP^TM) technology 

1.03	REFERENCES
A.	CE - European Union Compliance (CE)
B.	RoHS - Restriction of Use of Hazardous Substances
C.	WEEE - Waste Electrical and Electronic Equipment Directive
D.	UL, cUL - Underwriters Laboratory
E.	RFC - Request for Comments
F.	IEEE - Institute of Electrical and Electronics Engineers
G.	EN/IEC - International Electrotechnical Commission

1.04	SYSTEM DESCRIPTION
A.	Performance Requirements: Provide 1 Ethernet extended distance 10/100BaseT port and 1 10/100Base-TX standard port.
B.	The system shall utilize TIA/EIA 568-B cable connected to an RJ45 plug for standard Ethernet.
C.	The system shall utilize a BNC 1978 standard IEC 169-8 connector for extended transmission.

1.05	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed installation and operating information
B.	Warranty: Manufacturer’s Printed Warranty

1.06	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate controlled environment. 
B.	Storage Temperature not to exceed: -40˚C to +85˚C

1.07	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of -40˚C to +75˚C without the assistance of fan-forced cooling.
B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 90% (non-condensing). 

1.08	WARRANTY
A.	Limited Life Time Warranty: Vigitron guarantees product to be free of defects for product lifetime, defined as the time that product is in production plus 3 years from end of production.

PART 2 – PRODUCTS

2.1	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc. 7810 Trade Street, Suite 100, San Diego, CA 92121, USA 
2.	Phone 1-858-484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted

2.2	MANUFACTURED UNITS
A.	Reference Table A: Product Number, Descriptions and Maximum Distance
B.	Reference Table B: IEEE Product Compatibility Chart
C.	Reference Table C: Product System Compatibility Chart

2.3	GENERAL SPECIFICATIONS
A.	The 1-port Coax Ethernet extender shall be Vi2401A. 
B.	Standard Ethernet Ports:
1.	The device shall have one 10/100BaseT standard Ethernet ports in a compact housing:
a.	The Ethernet port will comply with: 
i.	IEEE 802.3u 10baseT 
ii.	IEEE 802.3u 100baseT 
2.	The Standard Ports will be compliant to IEC 60603-7.
3.	The device shall support Standard Ethernet UTP connection distances up to 100 meters.
4.	The device will be compliant to 802.3af and 802.3at Type 1 and 2 standards.
5.	The device will have 1 switch setting for Master/Slave.
6.	The Bandwidth selection will be done by automatic detection.
7.	The device shall be used as either transmitter or receiver in the same system.
C.	The Extended Distance Ethernet Ports:
1.	Will support distances up to 5,000 feet (1,524m) at 10BaseT. 
2.	Will support distances up to 1,800 feet (548m) at 100BaseT. 
3.	Will support the ability to pass 802.3af/at PoE from a source to a device at the stated distances. 
4.	Will support 10/100BaseT and PoE at following distances:
a.	802.3af at 1,500 feet (457m)
b.	802.3at at 500 feet (152m)
8.	Will maintain all 802.3af/at safety standards for PSE and PD communications. “5.”
D.	The system will provide the ability to test and verify connection status, and operating bandwidth between two transceivers over the extended connection.
E.	The device will be powered by a 12VDC, 24VAC or PoE. 
F.	Unit will consume less than 1.5 watts of power when external power is used and 1.8 watts when PoE is provided.
G.	The device shall provide below LED indicators for monitoring proper system operation:
1.	Power - Red indicates power on
2.	Extended distance traffic/Link – Orange
a.	Off - No traffic
b.	Flashing – Traffic
3.	Extended Bandwidth indication:
a.	10BaseT - Green indicating 10BaseT
b.	100BaseT - Orange indicating 100BaseT
4.	Standard Ethernet Connections: Green
a.	Off indicating no connection 
b.	Flashing - connection with traffic
5.	Standard Ethernet Bandwidth indication
a.	10/100BaseT Yellow
b.	Off - no connection 
c.	On - connection is valid
H.	The device shall be equipped with a 2 position switch: 
1.	Off position will note unit functioning as Slave
2.	On position will note unit functioning as Master
K.	The unit will automatically sense the optimum bandwidth and adjust accordingly.

2.4	DATA SPECIFICATIONS
A.	Data Interface: Passage of data compliant to: 
1.	RFC 768 UDP
2.	RFC 2068 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 1783 TFTP
6.	RFC 894 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Data Rate: 10/100 Mbps
C.	Data Connections: 1 standard Ethernet ports and 1 extended Ethernet ports

2.5	Vi2401A SPECIFICATIONS and FEATURE SETS
A.	The extender device will transmit and receive data using Symmetric Bandwidth (SBW™). 
1.	Bandwidth will be constant over the quoted extended distance with no more than a 5% decrease, when the input signal varies from a size of 64 bytes to 4500 bytes using bidirectional transmission.
2.	Bandwidth will be constant over the quoted extended distance with no more than 5% decrease when: 
a.	Bidirectional signals are transmitted with a packet size of 4,500 bytes.
b.	Unidirectional signals are transmitted with a packet size of 9,000 bytes.
c.	Bandwidth will remain the same for both upload and download operation.
B.	Packet losses will be at 2% or less at packet sizes, ranging from 64 bytes to 4,500 bytes bidirectional and 9,000 bytes unidirectional.
C.	Packet losses will be at 2% or less at packet sizes of 4,500 in bidirectional transmission.
D.	Packets per second (PPS) will not vary more than 5% at packet sizes from 64 to 4,500 bytes.
E.	Packet per second (PPS) will not vary more than 5% at packet of 4500 bytes in bidirectional transmission.
F.	Maximum distance will be 5,000 feet (1,524m) at 10BaseT. 
G.	Maximum distance will be 1,800 feet (548m) at 100BaseT. 
H.	Extender device must have the ability to function as Transceiver. 
I.	Extender device must have the ability to be powered using IEEE 802.3at or IEEE 802.3af PoE. 
J.	Extender device must have the ability to operate using Pass Through PoE (PTP™) with a single PoE source, providing power to both transceivers and PD device conforming to 802.3af/at standards. 
K.	Extender device must have the ability to pass through PoE functionality in compliance with IEEE 802.3af/at standards when communicating with a PD: 
1.	Pass through detection pulses from PSE to PD.
2.	Pass through classification pulses from PSE to PD.
3.	Pass through required power from PSE to PD. 
4.	Ability to provide Class 2 802.3af at maximum extended distance to both transceivers and PD from a PoE source. 
5.	Ability to provide Class 0, 1, 2, 3 and 4 802.3af/at power to both transceivers and PD from a PoE source depending on cable length.
L.	Extender must be able to operate in extended temperature environments of -40˚C to +75˚C type tested in compliance to NEMA-TS2 testing procedures.
M.	Extender must provide the ability to test extended distance connection continuity and bandwidth by means of LED indicators. 
2.6	CONNECTORS
A.	Power: IEC380-8 inlet 
B.	Extended Transmission Port: BNC 1978 standard, IEC 169-8
C.	Ethernet Port: RJ-45 : IEC 60603-7

2.7	ELECTRICAL SPECIFICATIONS
A.	Power Inputs
1.	12 Volts D.C  @ 150 mA
2.	24 Volts A.C  @ 80 mA
3.	PoE  used 1.8W max 

2.8	MECHANICAL SPECIFICATIONS
A.	Surface Mount Dimensions (H x W x L) 1.15” x 1.6” x 3.73” (3.0cm x 4.0cm x 9.5cm)
B.	Finish: Device shall be constructed of a metal enclosure. 
C.	Weight 0.212lb (96g)

2.9	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temp: -40˚C to +75 ˚C
B.	Storage Temp: -40˚C to +85˚C
C.	Relative Humidity: 0% to 90% (non-condensing)

2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS
A.	FCC Part 15, Subpart B, Class B 2010
B.	Emission Standards: 
1.	FCC Part 15, Subpart B, Class B 2010
2.	EN 55022:206+A1:2007
3.	EN61000-3-2:2006+A1:2009+A2:2009
4.	EN 61000-3-3:2008
5.	EN55024:1998+A1:2001+A2:2003
C.	Safety:
1.	CSA C22.2 NO. 60950-1-07-CAN/CSA INFORMATION TECHNOLOGY EQUIPMENT SAFETY PART GENERAL REQUIREMENTS - Edition 2 - Revision Date 2011/12/19
2.	UL 60950-1 INFORMATION TECHNOLOGY EQUIPMENT - SAFETY - PART 1: GENERAL REQUIREMENTS - Edition 2 - Revision Date 2011/12/19
D.	RoHS
E.	CE

2.11	ACCESSORIES
A.	Operation Manual
B.	2-pin Terminal block to round connector adapter 

2.12	MANUFACTURED UNITS REFERENCE TABLES

PRODUCT | DESCRIPTION | MAX. DISTANCE*

Vi2401A

Ethernet Extender over Coax

5,000 Feet (1,524m) @ 10BaseT
1,800 Feet (548m) @ 100BaseT

Table A: Product Number Descriptions
*Distance and performance figures are obtained using in-house testing mirroring typical installations. Factors such as cabling, connections, use of power and environmental conditions may affect actual distance, and should be taken in consideration.

PRODUCT | | COMPATIBLE IEEE STANDARDS

Vi2401A

IEEE 802.3u     IEEE 802.3af      
IEEE 802.3at

Fast Ethernet standard for 10/100TX
Power over Ethernet
Power over Ethernet

Table B: Product IEEE Compatibility Chart 

PRODUCT | COMPATIBLE ETHERNET EQUIPMENT

Vi2401A

Vi2400A Single port Mini Coax Ethernet Extender
Vi2400WP Weatherproof IP67 Coax Ethernet Extender
Vi2404A 4-port Coax Ethernet Extender
Vi2408A 8-port Coax Ethernet Extender
Vi2416A 16-port Coax Ethernet Extender
Vi2601 Single port Extended Coax Midspan
Vi2608 8-port Extended Coax Midspan
Vi2616 16-port Extended Coax Midspan

Table C: Product System Compatibility Chart

Vigitron reserves the right to change products or specifications without notice

END OF SECTION