DIVISION 27 21 29
Vi3405 MaxiiNet™ 5-Port Coax PoE Switch
PART 1 - GENERAL
1.01	SUMMARY
5-port PoE network switch with 4 extended coax network ports

1.02	SECTION INCLUDES
A.	Vi3405 MaxiNet™ 5-Port Coax PoE Switch 

1.03	REFERENCES
A.	CE - European Union Compliance (CE)
B.	RoHS - Restriction of Use of Hazardous Substances
C.	WEEE - Waste Electrical and Electronic Equipment Directive
D.	UL, cUL - Underwriters Laboratory
E.	RFC - Request for Comments
F.	IEEE - Institute of Electrical and Electronics Engineers
G.	EN/IEC - International Electrotechnical Commission

1.04	SYSTEM DESCRIPTION
A.	Performance Requirements: 4 Ethernet extended over Coax distance 10/100Base-T ports 
B.	Performance Requirements: 1 RJ45 connector standard Ethernet distance 328 feet (100m) 
C.	Performance Requirements: 1 MSA SFP Compatible stock
D.	The system shall utilize TIA/EIA 568-B cable connected to an RJ45 plug for standard Ethernet.
E.	The system shall utilize a BNC 1978 standard IEC 169-8 connector for extended transmission:
1.	The Vi3405 shall have 4 BNC connectors for extended transmission.
F.     The system shall utilize a circular power connector. 

1.05	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed installation and operating information
B.	Warranty: Manufacturer’s Printed Warranty

1.06	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate controlled environment. 
B.	Storage Temperature not to exceed: -40˚C to +85˚C

1.07	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of -30˚C to +75˚C without the assistance of fan-forced cooling.
B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 95% (non-condensing). 

1.08	WARRANTY
A.	Limited Lifetime Warranty: Vigitron guarantees product to be free of defects for product lifetime, defined as the time that product is in production plus 3 years from end of production.

PART 2 - PRODUCTS
2.01	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc. 7810 Trade Street, Suite 100, San Diego, CA 92121, USA 
2.	Phone 1-858-484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted

2.02	MANUFACTURED UNITS
A.	Reference Table A: Product Number, Descriptions and Maximum Distance
B.	Reference Table B: IEEE Product Compatibility Chart
C.	Reference Table C: Product System Compatibility Chart

2.03	GENERAL SPECIFICATIONS
A.	The device will include 5 active ports: 4 Coax port and 1 10/100Base-T standard Ethernet ports. 
B.	Standard Ethernet Ports:
1.	The device shall have one 10/100Base-T standard Ethernet ports in a compact housing:
a.	The Ethernet port will comply with: 
i.	IEEE 802.3u 10Base-T 
ii.	IEEE 802.3u 100Base-T 
2.	The standard ports will be compliant to IEC 60603-7.
3.	The SFP stock will be compliant to the MSA standard.
4.	The device shall support standard Ethernet UTP connection distances up to 328 feet (100m).
5.	The device will be compliant to IEEE 802.3af and IEEE 802.3at Type 1 and 2 standards.
6.	The device will have no switch settings.
7.	The bandwidth selection will be done by automatic detection.
8.	The PoE will be automatically detected 
9.	The device shall be used at the headend.
C.	Each extended distance ethernet ports:
1.	Will support distances up to 5,000 feet (1,524m) at 10Base-T. 
2.	Will support distances up to 1,800 feet (548m) at 100Base-T. 
3.	Will support the ability to pass 802.3af/at PoE from a source to a device at the stated distances. 
4.	Will support 10/100Base-T and PoE at following distances:
a.	IEEE 802.3af at 1,500 feet (457m)
b.	IEEE 802.3at at 500 feet (152m)
5.	Will maintain all IEEE 802.3af/at safety standards for PSE and PD communications. 
6.	Will accept SFP compliant to the MSA standard.
F.	The system will provide the ability to test and verify connection status and operating bandwidth between two transceivers over the extended connection.
G.	The device will be powered by the Vi1120 external power supply operating at 120W @ 57V. 
1.	The device will consume less than 8W
2.	The device will have the ability to provide PoE to each of 4 extended ports when powered locally.
H.	The device shall provide below LED indicators for monitoring proper system operation 1 per each of four extended ports:
1.	PoE  - Green indicates the presence of PoE 
2.	Link/Activity Yellow indicates link is presence and activity is taking place.
3.	10/100- (Green/Orange) indicates 10Mbps (Green) 100Mbps (Orange) 
a)	Off - No Connection 
b)	Flashing - Connection with Traffic

4.	 One Standard Ethernet Bandwidth Indication
a.	10/100Base-T Yellow
b.	Off - No Connection 
c.	On - Connection Is Valid
2.04	DATA SPECIFICATIONS
A.	Data Interface: Passage of data compliant to: 
1.	RFC 768 UDP
2.	RFC 2068 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 1783 TFTP
6.	RFC 894 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Data Rate: 10/100Mbps
C.	Data Connections: 1 Standard Ethernet Ports and 4 Coax Ethernet Ports

2.05	Vi3405 SPECIFICATIONS and FEATURE SETS
A.	The extender device will transmit and receive data using Symmetric Bandwidth (SBW™). 
1.	Bandwidth will be constant over the quoted extended distance with no more than a 5% decrease, when the input signal varies from a size of 64 bytes to 1,538 bytes using bidirectional transmission.
2.	Bandwidth will be constant over the quoted extended distance with no more than 5% decrease when: 
a.	Bidirectional signals are transmitted with a packet size of 1,538 bytes.
b.	Bandwidth will remain the same for both upload and download operation.
B.	Packet losses will be at 2% or less at packet sizes, ranging from 64 bytes to 1,538 bytes bidirectional.  
C.	Packet losses will be at 2% or less at packet sizes of 1,538 in bidirectional transmission.
D.	Packets per second (PPS) will not vary more than 5% at packet sizes, ranging from 64 bytes to 1,538 bytes.
E.	Packet per second (PPS) will not vary more than 5% at packet of 1,538 bytes in bidirectional transmission.
F.	Maximum distance will be 5,000 feet (1,524m) at 10Base-T. 
G.	Maximum distance will be 1,800 feet (548m) at 100Base-T. 
H.	Extender device must have the ability to function as Transceiver. 
I.	Extender device must have the ability to be powered using IEEE 802.3at or IEEE 802.3af PoE. 
J.	Extender device must have the ability to operate using Pass-Through-PoE (PTP™) from each port, providing power to both transceivers and PD device conforming to 802.3af/at standards. 
K.	Extender device must have the ability to pass through PoE functionality in compliance with IEEE802.3af/at standards when communicating with a PD: 
1.	Pass through detection pulses from PSE to PD.
2.	Pass through classification pulses from PSE to PD.
3.	Pass through required power from PSE to PD. 
4.	Ability to provide Class 2 IEEE 802.3af at maximum extended distance to both transceivers and PD from a PoE source. 
5.	Ability to provide Class 0, 1, 2, 3 and 4 IEEE 802.3af/at power to both transceivers and PD from a PoE source depending on cable length.
6.	Ability to provide up to 37 watts per power depending on input PoE power.
7.	Ability to allocate port power level based on “Smart Allocation” starting with port 1 as the highest priority.
L.	Extender must be able to operate in extended temperature environments of -30˚C to +75˚C type tested in compliance to NEMA-TS2 testing procedures.
M.	Extender must provide the ability to test extended distance connection continuity and bandwidth by means of LED indicators. 

2.06	CONNECTORS
A.	Power: Circular Power Connector 
B.	Data:
1.	Extended Ethernet connector to be 75 ohm BNC.
2.	Standard Ethernet connector to be compliant to IEC 60603-7.
3.	MSA Compliant Socket

2.07	ELECTRICAL SPECIFICATIONS
A.	Power Supply:
1.	The Vi3405 with 120W @ 57VDC, will operate and provide up to 37W per port 
2.	The Vi3405 with +12VDC @ 1A, will operate as a network switch but not provide PoE
3.	The Vi3405  with PoE will provide power at each port dependent on power provided.

2.08	MECHANICAL SPECIFICATIONS
A.	Dimensions (H x W x L): 1.2 x 3.75 x 5.1 in ; 3.0 x 9.5 x 13 cm
B.	Finish: Device shall be constructed of an aluminum metal enclosure. 
C.	Weight: 0.76 lb; 344 g
D.	Mounting: Table top or wall mount 

2.09	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temperature: -30˚C to +75˚C
B.	Storage Temperature: -40˚C to +85˚C
C.	Relative Humidity: 0% to 95% (non-condensing)

2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS
A.	FCC Part 15, Subpart B, Class B 2010
B.	Emission Standards: 
1.	FCC Part 15, Subpart B, Class B 2010
2.	EN 55022:206+A1:2007
3.	EN61000-3-2:2006+A1:2009+A2:2009
4.	EN 61000-3-3:2008
5.	EN55024:1998+A1:2001+A2:2003
D.	RoHS
E.	CE

2.11	ACCESSORIES
A.	Operation Manual 

2.12	MANUFACTURED UNITS REFERENCE TABLES

Table A: Product Number Descriptions
PRODUCT	DESCRIPTION	MAX. DISTANCE*	
Vi3405  
	5-port PoE network switch with 4 extended coax network ports
	5,000 Feet (1,524m) @ 10Base-T
1,800 Feet (548m) @ 100Base-T	
*Distance and performance figures are obtained using in-house testing mirroring typical installations. Factors such as cabling, connections, use of power and environmental conditions may affect actual distance, and should be taken in consideration.
Table B: Product IEEE Compatibility Chart 
PRODUCT		COMPATIBLE IEEE STANDARDS	
Vi3405  
	IEEE 802.3u     IEEE 802.3af      
IEEE 802.3at	Fast Ethernet standard for 10/100TX
Power over Ethernet
Power over Ethernet	

Table C: Product System Compatibility Chart
PRODUCT	COMPATIBLE ETHERNET EQUIPMENT	
Vi3405	Vi2401A  1-port Coax Ethernet Extender 
Vi2400A  1-port Coax Ethernet Extender
Vi2400WP  1-port Weatherproof Coax Ethernet Extender	

Vigitron reserves the right to change products or specifications without notice.

END OF SECTION