Title: Vi2401 A&E specifications
Author: Neil Heller
Last saved by: ali
Company: HP

DIVISION 27 21 29
Vi50001 1000Base-FX – 100/1000Base-TX Ethernet Media with built in PoE PD  

PART 1 - GENERAL
1.01	SUMMARY
A.	Vigitron Vi50001 is a PoE powered fiber to copper Ethernet media convertor.
1.02	SECTION INCLUDES
A.	Vigitron Vi50001 100/1000Base-TX Ethernet Convertor MM/SM compatible up to 80km, depending on the SFP used with ability to be powered by local 12VDC or PoE.
1.03	REFERENCES
A.	CE - European Union Compliance (CE)
B.	RoHS – Restriction of Use of Hazardous Substances
C.	WEEE – Waste Electrical and Electronic Equipment Directive
D.	RFC - Request for Comments 
E.	IEEE - Institute of Electrical and Electronics Engineers
F.	EN/IEC - International Electrotechnical Commission
1.04	SYSTEM DESCRIPTION
A.	The Vi50001 will function as a Layer 2 PoE powered network switch. 
1.05	Performance Requirements 
A.	Performance Requirements: (1) 100/1000Base-Tx copper port powered from a direct 12VDC power source or IEEE 802.3af (15.4W) / IEEE 802.3at (30W) compliant Power over Ethernet (PoE) Power Source (PSE). The device will have the ability to convert transmission from Fiber to Copper.  
1.	The system shall utilize a Small Format Pluggable (SFP) socket that conforms to the Multi Standards Agreement (MSA). The Vi50001 will be able to accept all forms of SFPs which conform to the MSA standards. 
1.	The system shall utilize EIA568, category 5/5e/6, 4-pair cables for 10Base-T, 100Base-TX or 1000Base-Tx. 
2.	Supports Jumbo Frames up to 9,000 bytes.
3.	Perform bidirectional conversion between fiber and copper transmission mediums. 
4.	The device will be able to accept power from a 12VDC @ greater at 1A power source.
5.	The device will be able to accept power from an IEEE 802.3.at PoE compliant source.

1.06	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed installation and operating information.
B.	Warranty: Manufacturer’s Printed Warranty
1.07	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate controlled environment. 
B.	Storage temperature not to exceed: -40˚C to +85˚C 
1.08	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of -40˚C to +80˚C without the assistance of fan-forced cooling.
B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0˚C to 95˚C (non-condensing). 
1.09	WARRANTY
A.	Vigitron Return and Warranty Policy: Vigitron warrants the product to be free of factory defects for the production lifetime of the product plus 3 years.
PART 2 - PRODUCTS
2.01	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc.: 7810 Trade St., San Diego, CA 92121, USA 
2.	Phone: +1 (858) 484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted
2.02	MANUFACTURED UNITS
A.	Model Number Descriptions: Reference Table A: Product Number Descriptions 
B.	Model Compatibility Chart: Reference Table B: Product Compatibility Chart
C.	Optional Accessories: Reference Table C: Optional Accessories Chart 
2.03	GENERAL SPECIFICATIONS
A.	The 100/1000Base-TX PoE media convertor to Fiber SFP shall be Vigitron Vi50001. 
B.	The Vi50001 shall comply with MSA standards for SFP.
C.	The Vi50001 shall support the following standards:
1.	Ethernet data IEEE 802.3/802.3u 100Base-TX and 1000BaseT, 802.3z protocol using auto-negotiating and auto-MDI/MDI-X features.
2.	Ethernet copper PHY conforming to 100Base and 1000Base-FX.
3.	802.1Q Tagging
D.	The Vi50001 shall have the following performance:
1.	Non-blocking architecture
2.	288Kb packet buffer
3.	1K MAC address
4.	Support for flow control for full duplex (symmetric/asymmetric) and half duplex (collision/carrier base) operation
5.	9K jumbo frame packet transmission
E.	The Vi50001 shall receive PoE power over Cat 5/5e cable to power itself.
F.	The Vi50001 shall detected by PoE IEEE 802.3af/at equipment automatically
G.	The Vi50001 shall support UTP distance up to 100m.
H.	The Vi50001 shall support the transmission of up to 1000Mbps over a single mode or multimode fiber, depending upon the SFP used.
I.	The Vi50001 shall provide power, fiber port status, copper port status, and PoE in-use status to indicate the LEDs for monitoring proper system operation.
J.	The Vi50001 shall be able to:
1.	Accept a DC power source of 12VDC @ 1amp when no PoE is available.
2.	Be powered by 802.3af PoE source when no external power source is available.
2.04	Ethernet DATA SPECIFICATIONS
A.	Data Interface: Ethernet IEEE 802.u 
B.	Data Rate: 10/100/1000 Mbps
C.	Connector: One RJ45 connector
D.	Operation Mode: Full Duplex / Half Duplex
2.05	OPTICAL SPECIFICATIONS
A.	Vigitron Vi50001
1.	Optical Fiber via SFP
a.	62.5/125um Multimode
b.	50/125um Multimode
c.	9/125um Multimode
2.	Number of Optical Ports: 1
3.	Number of Fibers Required
a.	Depends on SFP used
4.	Optical Wavelength: 1310nm and 850nm
5.	Optical Power Budget: Depends on SFP
6.	Maximum Distance: Depends on SFP

2.06	STATUS INDICATORS

A.	System
LED | COLOR | FUNCTION
PWR | Green | On

B.	10/100Base-TX Port
LED | COLOR | FUNCTION
LINK/ACT | Green | Blink
| | Lit
| | Off
PoE in Use | Green | Lit
| | Off

C.	100Base-SFP (This relates to function of main unit no SFP)
LED | COLOR | FUNCTION
LINK/ACT | Green | Blink
| | Lit
| | Off

2.07	CONNECTORS
A.	Power: 2-pin Terminal block
B.	Optical: Via MSA Compliant SFP Socket
C.	Data over Cat5/5e/6: RJ-45 connector
2.08	ELECTRICAL SPECIFICATIONS
A.	Power Input: 12VDC, Maximum power input 12VDC @ 1W
B.	The PoE input: IEEE 802.3af or IEEE802.3at (depending on the input power supply)
2.10	MECHANICAL SPECIFICATIONS
A.	Surface Mount Dimensions: 0.97 x 1.75 x 3.93 in.; 2.5 x 4.45 x 10 cm (HxWxL) 
B.	Finish: Module shall be constructed of a metal enclosure.
C.	Weight: 0.22 lbs (102g) 
2.11	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temp: -40°C to 80°C
B.	Storage Temp: -40°C to +85°C
C.	Relative Humidity: 0% to 95% (Non-condensing)
2.12	REGULATORY AGENCIES/APPROVALS AND LISTINGS 
A.	Federal Communications Commission (FCC) Part 15, Class A  
B.	European Union Compliance (CE) with the following standards:
1.	EN 55022:2006, Class A
2.	EN 61000-3-2:2006
3.	EN 61000-3-3+A2:2005
4.	EN 55024+A2:2003
C.	RoHS
D.	WEEE 
PART 3 - EXECUTION
3.01	PREPARATION
A.	Standalone Module (Surface Mount)
1.	Shall be mounted on a properly prepared surface adequate for the size and weight of the module. The placement of the unit shall allow provision for cable installation and maintenance as indicated on the approved detail drawings and in compliance with the installation manual.
B.	Optical Fibers
1.	Caution: NEVER look into the end of an active optical fiber when using a laser light output. Eye damage can occur. Wear eye protection when cleaving, terminating, and splicing the fiber.
2.	The number and type – Multimode / single mode of the optical fiber shall be the requirements of the selected SFP and used for both cable ends.
3.	All optical fiber cables shall be properly installed and terminated with the mating optical connectors.
4.	The optical connectors on the cable shall be cleaned in compliance to the optical connector manufacturer’s specifications and covered with dust caps until connection to the fiber optic module.

3.02	INSTALLATION
A.	General: The Vi50001 shall be installed in compliance with the Ethernet standards and is not to be more than 328 ft. (100m) away from the PoE powered device. 

3.03	MANUFACTURED UNITS REFERENCE TABLES

Vigitron Part No. | Description | Max. Distance*
Vi50001 | 10/100Base-TX to 100Base Fiber Media Convertor with Built-in 802.3at/802.3af PoE PD | Depending on the type of SFP and fiber cabling used
Table A: Product Number Descriptions 
* Maximum distance is limited to optical loss of the fiber and any additional loss by connectors, splices, and patch panels.

Vigitron Part No. | Compatible Ethernet Equipment

Vi50001

All products conform to:
•	Use of SFP conforming to MSA standards
•	Conforming to IEEE standards for Ethernet transmission
•	Conforming to IEEE standards for 802.3af PoE
•	Conforming to IEEE standards for 802.3at PoE

Table B: Product Compatibility Chart
Vigitron Part No. | Compatible Ethernet Equipment
Vi0012 | 12 VDC @ 1A power supply – for standard Vi50001 operation .
Vi00850MM-H | 850nm optical SFP for use on 50/125um and 62.5/125um multimode fiber.
Vi01310MM-H | 1310nm optical SFP for use on 50/125um and 62.5/125um multimode fiber.
Vi01310SM-H | 1310nm optical SFP for use on 9/125um single mode fiber.
Table C: Optional Accessories *

* Note: Optional Accessories are not required to operate the Vi5001. You may use other sources. However, Vigitron does not guarantee or warranty performance of products other than Vigitron labeled or provided.

Vigitron reserves the right to change products or specifications without notice.

END OF SECTION