Title: Vi1003M A&E Spec
Author: SW
Last saved by: Steve
Company: Vigitron
Document comments: Equivalent Specification to NVT-214-A-M or Nitek VB39M

Unshielded Twisted-Pair Video Transceiver 
Architecture and Engineering Bid Specification - Page  Vigitron Vi1003M or equivalent

TECHNICAL SPECIFICATIONS                                                   		SECURITY SYSTEM
DIVISION 16 - ELECTRICAL
SECTION 16770 - CLOSED CIRCUIT TELEVISION (CCTV) SYSTEM/ Cable Transmission and Reception Equipment

PART 2 – PRODUCTS                 

2.1	 GENERAL

A.	All equipment shall be standard components that are regularly manufactured and available.

B.	All systems and components shall have been tested and verified in actual use.

C.	All equipment shall be provided with the availability of a U.S.A toll-free technical support number from the manufacturer. The number shall provide technical assistance to the caller at no charge for as long as the product is installed.

2.2	UNSHIELDED TWISTED-PAIR PASSIVE VIDEO TRANSCEIVER

A.	The UTP Video Transceiver shall be capable of transmitting and receiving baseband monochrome or color video signals over unshielded twisted-pair (UTP) telephone wire to a passive transceiver up to a distance of 750 feet (229 m) without requiring power 
		
B.	If used as a Transmitter, Distances up to 3,000 feet (1914 m) shall be supported when used in conjunction with an approved active receiver, and support a minimum of 500 lines of video resolution.

C.	If used as a Transmitter, the device shall accept a baseband video signal, each from a 75-ohm source.

D.	If used as a Receiver, the device shall produce a baseband video signal capable of driving a 75-ohm load.

E.	Bi-directional signal transmission via the Vertical Interval of the video signal shall be supported up to 750 feet (229 m) when using this transceiver to transmit the signal to another passive receiver, so long as all other requirements are met. These signals are typically known as “Up the Coax” control, used to facilitate Pan/Tilt/Zoom functionality with the appropriate and compatible PTZ hardware.

F.	The transceiver shall have built-in differential transient protection without the need for a ground connection.

G.	The transceiver shall be equipped with corrosion-resistant screw terminals for connection to UTP wire.

H.	The transceiver housing shall be equipped with an integrated male BNC for 75-ohm camera connection.  

a.	The transceiver shall interlock directly to the BNC receptacle, without requiring additional mounting hardware

I.	The transceiver shall deliver signals operating in the same cable bundle as telephone, data, low voltage or other video signals, without interference.

J.	The transceiver shall meet or exceed the following performance specifications:
a.	Typical common-mode rejection of 60 dB between the frequencies of 15 KHz-5 MHz.
b.	The receiver device shall be compatible with NTSC, PAL and SECAM color video standards.
c.	Compatible with 0.6 to 1.6 Vpp composite color or black and white video signals into 75 Ohms.
d.	Frequency response from DC to 6 MHz.
e.	Typical Insertion Loss of 0.5 dB or better.
f.	Transient immunity of per IEEE Std C62.41, formerly known as IEEE Std 587 (IEEE Recommended Practice for Surge Voltages in Low-Voltage AC Power Circuits).
g.	The transceiver shall be suitable for indoor use or for outdoor use in an environmental enclosure at an operating temperature range –20 to 75 degrees Celsius. 

K.	The transceiver shall be compatible with 24-16 AWG UTP wire.

L.	The transceiver shall be compatible with Category 2 or better UTP wire at as specified in this document

M.	The transceiver shall weigh no more than 0.7 oz (20 g)

N.	The transceiver dimensions shall not exceed 1.26” x 0.94” x 0.55”, (32 mm, 23.9mm, 14 mm) 

O.	The transceiver shall be UL/cUL listed, and CE Compliant.

P.	The transceiver manufacturer shall provide a limited lifetime warranty.

Q.	The UTP passive video transceiver, shall be the :
a.	Vigitron Vi1003M or
b.	Equivalent product