Author: mngo
Last saved by: ali
Company: Hewlett-Packard Company

DIVISION 27 21 29
Vi3305 5-Port Extended UTP PoE Switch
PART 1 - GENERAL
1.01	SUMMARY
5-Port Extended UTP PoE Switch

1.02	SECTION INCLUDES
Vi3305 5-Port Extended UTP PoE Switch

1.03	REFERENCES
A.	CE - European Union Compliance (CE)
B.	RoHS - Restriction of Use of Hazardous Substances
C.	WEEE - Waste Electrical and Electronic Equipment Directive
D.	RFC - Request for Comments
E.	IEEE - Institute of Electrical and Electronics Engineers
F.	EN/IEC - International Electrotechnical Commission

1.04	SYSTEM DESCRIPTION
A.	Performance Requirements: 4 Ethernet extended distance 10/100Base-T ports
B.	Performance Requirements: 1 RJ45 connector standard Ethernet distance 328 feet (100m) 
C.	Performance Requirements: 1 MSA SFP Compatible socket
D.	The system shall utilize TIA/EIA 568-B cable connected to an RJ45 plug for standard Ethernet.
E.     The system shall utilize a circular power connector. 

1.05	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed Installation and Operating Information
B.	Warranty: Manufacturer’s Printed Warranty

1.06	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate controlled environment. 
B.	Storage temperature not to exceed: -40˚C to +85˚C

1.07	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of -30˚C to +75˚C without the assistance of fan-forced cooling.
B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 95% (non-condensing). 

1.08	WARRANTY
A.	Limited Lifetime Warranty: Vigitron guarantees product to be free of defects for product lifetime, defined as the time that product is in production plus 3 years from end of production.

PART 2 - PRODUCTS
2.01	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc. 7810 Trade Street, Suite 100, San Diego, CA 92121, USA 
2.	Phone 1-858-484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted

2.02	MANUFACTURED UNITS
A.	Reference Table A: Product Number, Descriptions and Maximum Distance
B.	Reference Table B: IEEE Product Compatibility Chart
C.	Reference Table C: Product System Compatibility Chart

2.03	GENERAL SPECIFICATIONS
A.	The device will contain 5 active ports: Four extended Ethernet ports and one 10/100Base-T standard Ethernet port.
B.	Standard Ethernet Port:
1.	The device shall have one 10/100Base-T standard Ethernet port
a.	The Ethernet port will comply with: 
i.	IEEE 802.3u 10Base-T 
ii.	IEEE 802.3u 100Base-T 
2.	The standard ports will be compliant to IEC 60603-7.
3.	The SFP stock shall be compliant to the MSA standard.
4.	The device shall support standard Ethernet UTP connection distances up to 328 feet (100m).
5.	The device shall have no switch settings.
6.	The bandwidth selection shall be done by automatic detection.
7.	The device shall be used at the headend.
C.	Each extended distance ethernet ports:
1.	Shall support distances up to 3,000 feet (909m) at 10Base-T. 
2.	Shall support distances up to 2,000 feet (606m) at 100Base-T. 
3.	Shall support 10/100Base-T and PoE at following distances:
a.	IEEE 802.3af at 2,000 feet (909m)
b.	IEEE 802.3at at 800 feet (242m)
4.	Shall provide up to 50W at a distance of 750 feet (228m) when used with Vi2300 series.
5.	Shall maintain all IEEE 802.3af/at safety standards for PSE and PD communications. 
6.	Shall support SFP compliant to MSA standards.
F.	The system shall provide the ability to test and verify connection status and operating bandwidth between two transceivers over the extended connection.
G.	The device shall be powered by the Vi1120 external power supply operating at 120W @ 57V. 
1.	The device shall consume less than 8W.
2.	Shall have the ability to provide PoE to each of 4 extended ports. The device shall provide below LED indicators for monitoring proper system operation 1 per each of four extended ports:
a.	PoE  - (Green) indicates the presence of PoE 
b.	Link/Activity-(Yellow flashing) indicates the link is presence and activity is taking place.
i.	10/100- (Green) indicates 10Mbps or (Orange) 100Mbps 
ii.	Off - No Connection
c.	One Standard Ethernet Bandwidth indication
i.	10/100Base-T Yellow
ii.	Off - No Connection 
iii.	On - Connection is Valid
2.04	DATA SPECIFICATIONS
A.	Data Interface: Passage of data compliant to: 
1.	RFC 768 UDP
2.	RFC 2068 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 1783 TFTP
6.	RFC 894 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Data Rate: 10/100Mbps
C.	Data Connections: 
1.	1 standard Ethernet ports and 4 extended Ethernet ports

2.05	Vi3405 SPECIFICATIONS and FEATURE SETS
A.	The extender device shall transmit and receive data using Symmetric Bandwidth (SBW™). 
1.	Bandwidth shall be constant over the quoted extended distance with no more than a 5% decrease, when the input signal varies from a size of 64 bytes to 1,538 bytes using bidirectional transmission.
2.	Bandwidth shall be constant over the quoted extended distance with no more than 5% decrease when: 
a.	Bidirectional signals are transmitted with a packet size of 1,538 bytes.
b.	Bandwidth shall remain the same for both upload and download operation.
B.	Packet losses shall be at 2% or less at packet sizes, ranging from 64 bytes to 1,538 bytes bidirectional.  
C.	Packet losses shall be at 2% or less at packet sizes of 1,538 in bidirectional transmission.
D.	Packets per second (PPS) shall not vary more than 5% at packet sizes, ranging from 64 bytes to 1,538 bytes.
E.	Packet per second (PPS) shall not vary more than 5% at packet of 1,538 bytes in bidirectional transmission.
F.	Maximum distance shall be 3,000 feet (909m) at 10Base-T for each of 4 extended ports.  
G.	Maximum distance shall be 2,000 feet (606m) at 100Base-T for each of 4 extended ports.
H.	The device must have the ability to be powered using IEEE 802.3at or IEEE 802.3af PoE. 
I.	The device must have the ability to provide IEEE 802.3af/at up to 36W to each port.
J.	The device must have the ability to allocate port power level based on “Smart Allocation” starting with port 1 as the highest priority. 

K.	The device must be able to operate in extended temperature environments of -30˚C to +75˚C type tested in compliance to NEMA-TS2 testing procedures.

2.06	CONNECTORS
A.	Power: Circular power connector 
B.	Data:
1.	Extended Ethernet: RJ45 connector compliant to IEC 60603-7.
2.	Standard Ethernet: RJ45 connector compliant to IEC 60603-7.
3.	MSA Compliant SFP Socket

2.07	ELECTRICAL SPECIFICATIONS
A.	Power Supply:
1.	Vi1120 (120W @ 57VDC), Vi3305 shall operate and provide up to 37W per port 
2.	Vi0012 ( +12VDC @ 1A), Vi3305 shall operate without PoE
2.08	MECHANICAL SPECIFICATIONS
A.	Dimensions (H x W x L): 1.2 x 3.75 x 5.1 in ; 3.0 x 9.5 x 13 cm
B.	Finish: Device shall be constructed of an aluminum metal enclosure. 
C.	Weight: 0.76 lb, 344g
D.	Mounting: Table top or wall mount 

2.09	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temperature: -30˚C to +75˚C
B.	Storage Temperature: -40˚C to +85˚C 
C.	Relative Humidity: 0% to 95% (non-condensing)

2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS
A.	FCC Part 15, Subpart B, Class B 2010
B.	Emission Standards: 
1.	FCC Part 15, Subpart B, Class B 2010
2.	EN 55022:206+A1:2007
3.	EN61000-3-2:2006+A1:2009+A2:2009, EN 61000-3-3:2008
4.	EN55024:1998+A1:2001+A2:2003
D.	RoHS
E.	CE

2.11	ACCESSORIES
A.	Operation Manual 
B.	DIN Rail Mounting Brackets

2.12	MANUFACTURED UNITS REFERENCE TABLES

Table A: Product Number Descriptions
PRODUCT | DESCRIPTION | MAX. DISTANCE*

Vi3305

Ethernet Extender over Coax

3,000 Feet (909m) @ 10Base-T
2,000 Feet (606m) @ 100Base-T

*Distance and performance figures are obtained using in-house testing mirroring typical installations. Factors such as cabling, connections, use of power and environmental conditions may affect actual distance, and should be taken in consideration.

Table B: Product IEEE Compatibility Chart
PRODUCT | | COMPATIBLE IEEE STANDARDS

Vi3305

IEEE 802.3u     IEEE 802.3af      
IEEE 802.3at

Fast Ethernet standard for 10/100TX
Power over Ethernet
Power over Ethernet

Table C: Product System Compatibility Chart
PRODUCT | COMPATIBLE ETHERNET EQUIPMENT

Vi3305

Vi2300A   1-Port Mini UTP Ethernet Extender 
Vi2301A   1-Port UTP Ethernet Extender
Vi2304A   4-Port UTP Ethernet Extender
Vi2308A   8-Port UTP Ethernet Extender
Vi2316A   16-Port UTP Ethernet Extender

Vigitron reserves the right to change products or specifications without notice.

END OF SECTION