Title: Vi2401 A&E specifications
Author: Neil Heller
Last saved by: ali
Company: HP

DIVISION 27 21 29
Vi2608 8-port Extended Coax Managed High Power PoE Midspan
PART 1 - GENERAL
1.01	SUMMARY
A.	8-port Managed Coax PoE Midspans
1.02	SECTION INCLUDES
A.	Vi2608: 8-port Managed Coax PoE Midspans
1.03	REFERENCES
A.	European Union Compliance (CE)
B.	RoHS
C.	WEEE compliant 
D.	UL 
1.04	SYSTEM DESCRIPTION
A.	Performance Requirements: Provide 8-port PoE power at IEEE 802.3af/at up to 36W.
B.	The system shall utilize TIA/EIA 568-B cable connected to an RJ-45 plug.
C.	The system shall utilize 75 Ohm Coax cables for transmission of 10/100/1000baseT.
1.05	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed installation and operating information
B.	Warranty: Manufacturer’s printed warranty
1.06	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate controlled environment. 
B.	Storage temperature not to exceed: -30˚C to +70˚C.
1.07	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of -10˚C to +40˚C.
B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 90% (non-condensing). 
1.08	WARRANTY
A.	Limited Life Time Warranty: Vigitron guarantees the product to be free of defects for the product lifetime, defined as the time that the product is in production or 3 years, whichever is longer.
PART 2 - PRODUCTS
2.01	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc. 7810 Trade Street, Suite 100, San Diego, CA 92121, USA 
2.	Phone 1-858-484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted
2.02	MANUFACTURED UNITS
A.	Reference Table A: Product Number Descriptions and Maximum Distance 
B.	Reference Table B: IEEE Product Compatibility Chart
C.	Reference Table C: Product System Compatibility Chart 
2.03	GENERAL SPECIFICATIONS
A.	The Coax extended Midspan shall be Vi2616 for 16 ports. 
B.	Ethernet Port:
1.	The module shall support the Ethernet data IEEE 802.3/802.3u 10/100Base-TX protocol.
2.	The Ethernet port shall comply with: 
a.	IEEE 802.3 10baseT 
b.	IEEE 802.3u 100baseT
c.	Shall provide up to full 802.3af/at per port
3.	Standard ports shall be compliant to IEC 60603-7.
4.	The device shall support standard Ethernet UTP connection distances up to 328 ft. (100m).
C.	The Vi2608:
1.	Shall support the ability to provide 802.3af/at PoE power at the stated distances to a PD device.
2.	Shall maintain all 802.3af/at safety standards.
3.	Shall provide for a default setting without the need for operational programing for: 
a.	Recognition of PD device
b.	Recognition of PD device class
c.	Recognition of individual port failure mode
d.	Flash LEDs upon port failure
D.	Vi2608 shall provide operation management and monitoring via Windows™ software.
E.	Software and user program shall not be mandatory for operation.
F.	Computer connection to the Vi2608 shall be by means of:
1.	USB Connector: Direct USB 2.0 connection
2.	RJ-45 Connector: Ethernet network connection
G.	Software functions shall include: 
1.	Programming functions: 
a.	Port Priority
b.	Port Enable 
c.	Port Disable 
d.	Force Power 
e.	Inrush Power 
f.	Power Class 
g.	Auto Mode Operation
h.	Port Reset
i.	Single And Multiple Port Programming 
2.	Monitoring Functions shall include: 
a.	Port Status
b.	PD Type Identification
c.	Power Class Validation
d.	Port Voltage 
e.	Port Current 
f.	Port Temperature 
g.	Polling Status 
h.	System Power Allocation 
i.	System Power Delivery  
H.	The device shall provide below indicating LED’s for monitoring proper system operation:
1.	Red, Solid: Device Power On 
2.	Green, blink slow: Request power
3.	Green, solid: Power Present
4.	Green, blink fast: Fault condition
I.	Security shall be provided via the use of the client software. Access shall not be permitted without authorized use of the client software:
J.	Client software shall be Vi2200Vxx where xx shall stand for the version number 
K.	Client software shall be able to provide for automatic discovery of all Vi2208A/Vi2216A, Vi2508/Vi2516 and Vi2608/Vi2616 on the same network. 
1.	Client software: 
a.	Shall provide security access via the use of a user name and password.
b.	Shall provide the ability to display multiple Vi2608 operating on the same network.
c.	Shall provide the ability to access multiple Midspan units from a single screen. 
2.	The client software could be configured to provide SNMP output that is compatible with standard SNMP Traps. 
a.		The SNMP shall have the ability to provide the following messages: 
1.	SNMP Activated 
2.	SNMP Deactivated 
3.	Communication Error 
4.	Port idle with port number.
5.	Port power disabled with port number.
6.	Port power forced power with port number. 
7.	Port power required with port number. 
8.	Port number fault with fault codes.
b.		The SNMP shall have the ability to provide the following fault codes:
1.	MPS Absent 
2.	Short 
3.	Overload
4.	Power Denied 
5.	Thermal Shut Down
6.	Startup Failure 
7.	Classification Failure
c.	Clients operating on the same network with SNMP traps shall be able to receive messages from all Midspans, where the SNMP function is active without the need for the client software to display.
3.	Client software shall be able to provide a Stay Alive feature:
a.	Shall continuously ping each individual port for up to 50 units to determine its operating condition. 
b.	Shall report condition of port via GUI and/or SNMP 
c.	In the event the device connection is lost shall attempt to restore connection. 
4.	Client software shall provide the ability to send messages to both private and public email addresses
a.	Shall provide test set up configuration 
5.	Client software shall have the ability to run in the background of Windows™ based software without      interference to exiting software and provide alerts as to alarm conditions.	  
2.04	DATA SPECIFICATIONS
A.	Data Interface: Passage of data compliant to:
1.	RFC 768 UDP
2.	RFC 2068 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 1783 TFTP
6.	RFC 894 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Data Rate: 10/100/1000 Mbps
C.	Data Inputs: 
1.	8 standard Ethernet ports 
D.	Data Outputs: 
1.	9 extended Ethernet ports 
E.	Power Outputs: 
1.	PoE compliant to IEEE 802.3af up to 15.4W
2.	PoE compliant to IEEE 802.3at up to 36W Type 1 and Type 2
2.05	Vi2616 / SPECIFICATIONS AND FEATURE SETS 
A.	When used with the Vi2401A:
1.	At full IEEE 802.3af, the PoE power shall transmit to a PD at 1,800 ft. (606m).  
2.	At full IEEE 802.3at, the PD power shall transmit to a PD at 500 ft. (151m). 
B.	Must have the ability to provide full class 3 IEEE 802.3af and IEEE 802.3at PoE at each port without power sharing among ports. 
C.	Must have the ability to:
1.	Recognition a standard a PD
2.	Recognize and respond to a PD class
3.	Provide and monitor power to a PD
4.	Ability to cease power in the event of a shortage or other abnormal conditions at the load.
D.	Each port shall be protected electronically against over current conditions. 
E.	Each port’s status shall be monitored and logged. 
F.	In the event power is lost, on a per port bases, the unit shall have the ability to restart power automatically if the condition that caused loss of power is no longer present.
G.	Individual PoE port power shall be programmable up to 36W per port.

2.06	CONNECTORS
A.	Power: IEC380-8 Inlet 
B.	Ethernet: RJ-45, Standard Ethernet connector to be compliant to IEC 60603-7
C.	Ethernet and PoE: 75 Ohm BNC
D.	USB: Type B 
2.07	ELECTRICAL SPECIFICATIONS
A.	Power Inputs:
1.	110-230VAC/50-60Hz, auto-sensing
B.	Output power: 
1.	54VDC @ 36W per port, 300W aggregated
2.08	MECHANICAL SPECIFICATIONS
A.	Dimensions (H x W x L):
1.	1.75 x 17 x 12 in, 4.3 x 43 x 30.5 cm
B.	Finish: the device shall be constructed of a metal enclosure. 
C.	Weight 
1.	8lb, 3.6Kg 
D.	Mounting: 
1.	Vi2608 shall be rack mountable in a standard EIA 19” rack mount enclosure.

2.09	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temp: -10˚C to +40 ˚C
B.	Storage Temp: -30˚C to +70˚C
C.	Relative Humidity: 0% to 90% (Non-condensing)
2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS:
A.	CE
B.	RoHS Compliant 
C.	UL 60950-1, 2^nd Edition, 2007-03-27, CSA C 22.2 No. 60950-1-07 2^nd Edition, 2007-03
D.	FCC Part 15, Subpart B, Class B 2010
E.	Emission Standards: 
1.	EN 55022:206+A1:2007
2.	EN61000-3-2:2006+A1:2009+A2:2009
3.	EN 61000-3-3:2008
4.	EN55024:1998+A1:2001+A2:2003
2.11	ACCESSORIES
A.	Operation Manual 
B.	Windows™ set up software 

2.12	MANUFACTURED UNITS REFERENCE TABLES

Vi2600 Product Series | Description | Max. Distance*
Vi2608 | 8 port 802.3af/at Extended Coax Midspan | Depends on PD Power Requirement
Table A: Product Number Descriptions 
* Distance figures are obtained using in-house testing mirroring installation. Factors such as cabling, connections, use of power, and environmental conditions may affect the actual distance and should be taken in consideration.

Extended Ethernet Transceiver | Compatible IEEE Standards

Vi2608

IEEE 802.3u Ethernet standard for 10/100/1000TX protocol
IEEE 802.3af Power over Ethernet 
IEEE 802.3at Power over Ethernet; Type 1 and Type 2

Table B: Product IEEE Compatibility Chart

Extended Ethernet Transceiver | Compatible Ethernet Equipment

Vi2608

Vi2400A, Vi2400W, Vi2401A, Vi2404A, Vi2408A, Vi2416A 
Vi3205

Table C: Product System Compatibility Chart

Vigitron reserves the right to change products or specifications without notice.
END OF SECTION