Author: aeghbal aeghbal
Last saved by: ali

DIVISION 27 21 29
Vi3003WP IP67 Weatherproof 1G Drop and Insert 3-Port 60W PoE Switch
PART 1 - GENERAL
1.01	SUMMARY
A.	Ethernet  IP67 Weatherproof 1G Drop and Insert 3-Port 60W PoE Switch

1.02	SECTION INCLUDES
A.	Vi3003WP Ethernet  IP67 Weatherproof 1G Drop and Insert 3-Port 60W PoE Switch

1.1	REFERENCES
A.	CE - European Union Compliance (CE)
B.	RoHS - Restriction of Use of Hazardous Substances
C.	WEEE - Waste Electrical and Electronic Equipment Directive
D.	RFC - Request for Comments
E.	IEEE - Institute of Electrical and Electronics Engineers
F.	EN/IEC - International Electrotechnical Commission

1.2	SYSTEM DESCRIPTION
A.	Connection Requirements: Provide three IP67 RJ45 connections:
1.	The system shall utilize a Category 5/5e/6 cables terminated in an IP67 RJ45 connector with EIA568-B configuration for PoE and data in for standard 10Base-T or 100Base-T for network transmission ports.
2.	The system shall utilize a Category 5/5e/6 cables terminated in two IP67 RJ45 connector with EIA568-B configuration for PoE and data out for standard 10Base-T or 100Base-T for drop and insert ports.

1.3	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed Installation and Operating Instruction
B.	Warranty: Manufacturer’s Printed Warranty

1.4	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate-controlled environment.
B.	Storage temperature not to exceed: -40˚C to +85˚C.

1.5	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of -40˚C to +75˚C without the assistance of forced-air cooling.
B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 95% (non-condensing). 

1.6	WARRANTY
A.	Limited Lifetime Warranty: Vigitron guarantees product to be free of defects for product’s lifetime, defined as the time that product is in production plus 3 years from the end of production.

1.	1
2.	2

PART 2 - PRODUCTS
2.1	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc. 7810 Trade Street, Suite 100, San Diego, CA 92129, USA 
2.	Phone: 1-858-484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted

2.2	MANUFACTURED UNITS
A.	Reference Table A: Product Number, Descriptions and Maximum Distance
B.	Reference Table B: IEEE Product Compatibility Chart
C.	Reference Table C: Product System Compatibility Chart

2.3	GENERAL SPECIFICATIONS
A.	The Drop and Insert 3-Port Switch shall be the Vi3003WP.
B.	Ethernet Ports:
1.	The module shall support the Ethernet data IEEE 802.3/802.3u 10/100/1000Base-TX protocol with auto-sensing.
2.	Bandwidth settings will be automatically detected.
3.	Module will process Juimbo Frame packets up to 9,600 bytes at all speeds.
4.	The module features three fixed 10/100/1000TX electrical ports in a compact mini chassis. The Ethernet port will comply with:
i.	IEEE 802.3 10Base-T 
ii.	IEEE 802.3u 100Base-T 
iii.	IEEE 802.3ab 1000Base-T
5.	Ports 1, 2 and 3 will auto bandwidth configure to 10/100/100Base-TX.
6.	Ports will be compliant to IEC 60603-7.
7.	The module shall support standard Ethernet UTP connection distances up to 328 feet (100m) for all connections.
8.	Module will use Pass-Through PoE (PTP™) for PoE functions.
9.	The module will always provide 1000Base-T bandwidth for network connections.
C.	The Vi3003WP will be able to support:
1.	PoE power source of 74W: 
a.	Camera power at 60W using (1) modules at 428ft (130m) distance. 
b.	Camera power at 30W using (2) modules at 800ft (242m) distance. 
2.	PoE power source of 37W: 
a.	Camera power at 25.5W using (3) modules at 1,200ft (363m) distance. 
b.	Camera power at 12.94W using (7) modules at 2,500ft (757m) distance.
3.	PoE power source of 30W: 
a.	Camera power at 25.5W using (1) modules at 500ft (151m) distance.
b.	Camera power at 12.95W using (4) modules at 1,500ft (454m) distance.
c.	Camera power at 6.49W using (6) modules at 2,200ft (666m) distance.
4.	PoE power source of 15.4W: 
a.	Camera power at 12.94W using (1) modules at 500ft (151m) distance.
b.	Camera power at 6.94W using (5) modules at 1,800ft (545m) distance.
D.	Unit will support the ability to pass 802.3 af/at PoE from a source to a device at the stated distances to provide power to a PoE powered device.
E.	Unit will maintain all IEEE 802.3at PoE safety standards.
F.	Unit will have the ability to be powered from different PoE sources: IEEE 802.3af, IEEE 802.3at, 60W, and 74W.
G.	Unit will be able to accept an external power source up to 90W @ 57VDC and provide a 60W on the repeated output.
H.	Unit will be able to accept an external power input of 90W @ 57VDC and provide 60W and 30W at each of one port simultaneously 
I.	Unit will be able to provide up to 36W output for drop/repeater output.
J.	PoE loads are automatically sensed with no programming required.
K.	At any point, a qualified external power supply can be connected boosting the total PoE power output to 90W from that point.
L.	Unit will consume less than 4.0W when powered by PoE. 
M.	The module shall provide indicating LED’s for monitoring proper system operation.
1.	Network Status  
a.	Off – No Traffic; Indicated as LED in the “on” condition.
b.	On – Traffic Present; Orange LED with both sides of the RJ45 connector flashing.
2.	Power Level Indication: The module will be able to indicate the available power levels by means for LEDs: 
a.	30W: Orange – Status On 
b.	60W: Orange – Status On
3.	Traffic - Link and Activity. The module will have the following link and activity LED statuses and colors: 
a.	Port 1  
i.	1G - Green
ii.	Link – Yellow Steady On 
iii.	Activity - Yellow Flashing 
b.	Port 2 
i.	1G - Green
ii.	Link – Yellow Steady On 
iii.	Activity - Yellow Flashing 
c.	Port 3 
i.	1G - Green
ii.	Link – Yellow Steady On 
iii.	Activity - Yellow Flashing 

2.4	DATA SPECIFICATIONS
A.	Data Interface: Passage of data compliant to: 
1.	RFC 768 UDP
2.	RFC 2068 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 1783 TFTP
6.	RFC 894 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Data Rate: 10/100/1000Mbps
C.	Data Connections: 3
1.	Three IP67 RJ45 connectors conforming to IEC 60603-7

2.5	The Vi3003WP SPECIFICATIONS and FEATURE SETS
A.	Unit will be able to provide the following performance: 
1.	Bandwidth per module will be constant over the quoted extended distance with less than a one percent (1%) decrease.
2.	Latency per module will be no greater than 9.0us. 
B.	Packet losses per module will be less than one percent (1%) at 10,000 bytes.
C.	Packets per second (PPS) loss per module will be less than 1%.
D.	Unit will process Jumbo Frames wire speed performance up to 10,000 bytes.
E.	Unit will be able to connect and provide access up to nine (9) individual IP device addresses.
F.	Unit will function as a Layer 2 network switch with the following features:
1.	MDI-MDIX support
2.	TCP/IP Ingress Rate Detection
3.	802.1p
4.	IPVv4 TOS
5.	802.1Q VID
6.	802.1X Authentication
G.	Unit must have the ability to be powered using either IEEE 802.3at, IEEE 802.3af, and 74W PoE.
H.	Unit must have the ability to operate using Pass-Through-PoE (PTP^TM) with a PoE source that provides power to all modules in a single cable link and connected PoE powered device.
I.	Unit must have able to operate in extended temperate environments of -20˚C to 75˚C.
J.	Unit must provide the ability to display transmission connection continuity and bandwidth by means of LED indicators.

2.6	CONNECTORS
A.	Power Input: IP67 circular waterproof connector.
B.	Data: Three IP67 RJ45 Connectors

2.7	ELECTRICAL SPECIFICATIONS
A.	Power consumption: 4W
B.	PoE Input: IEEE 802.3af/at up to 74W
C.	PoE Output: IEEE 802.3af/at, UPoE up to 60W
D.	Local Power supply Input: 48-57VDC up to 90W

2.8	MECHANICAL SPECIFICATIONS
A.	Dimensions:  With connectors:1.82x2.75x10.34 in., 4.62x6.99x26.3 cm (HxWxL)
                            With no connectors 1.82x2.75x5.84 in., 4.62x6.99x14.84 cm (HxWxL)
B.	Finish: ABS plastic, UL rating of 94V-0 
C.	Weight: 1.27lb, 576g

2.9	ENVIRONMENTAL SPECIFICATIONS 
A.	Operating Temp: -40˚C to +75˚C 
B.	Storage Temp: -40˚C to +85˚C
C.	Relative Humidity: 0% to 95% (Non-condensing)

2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS 
A.	Emission Standards: 
1.	RFC 768 UDP, RFC 2068 HTTP
2.	RFC 793 TCP, RFC 791 IP
3.	RFC 1783 TFTP, RFC 894 IP over Ethernet
B.	RFC 2544 TCP/IP Packet Transmission
C.	RoHS
D.	CE
E.	WEEE

2.11	MANUFACTURED UNITS REFERENCE TABLES

Table A: Product Number Descriptions
PRODUCT | DESCRIPTION | MAX. DISTANCE*
Vi3003WP | Drop and Insert 60W PoE 3-Port Switch | 328 Feet (100m) @ 100Base-T
*Distance and performance figures are obtained using in house testing mirroring installation. Factors such as cabling, connections, use of power and environmental conditions may affect actual distance and should be taken in consideration. Distance represents single Device link.

Table B: Product IEEE Compatibility Chart
PRODUCT | | COMPATIBLE IEEE STANDARDS

Vi3003WP

IEEE 802.3u     IEEE 802.3af      
IEEE 802.3at
IEEE 802.3ab  
IEEE 802.3z
802.1p
802.1Q
802.1D
802.1s
802.3u
802.3x
802.3w

Fast Ethernet standard for 10/100TX
Power over Ethernet
Power over Ethernet
1000Mbps Ethernet

Table C: Product Data Interfaces and Compliances Chart
PRODUCT | DATA INTERFACES AND COMPLIANCES

Vi3003WP

RFC 768 UDO
RFC 2068 HTTP 
RFC 793 TCP
RFC791 IP 
RFC 1783 TFTP
RFC 894 894 IP over Ethernet 
RFC 2544 TCP/IP Packet Transmission

Table D: Product Service Compliance Chart
PRODUCT | SERVICE COMPLIANCES

Vi3003WP

IP v4 Type of Service (TOS) and Differential Diff-Serv
IPv6 Traffic Class

Vigitron reserves the right to change products or specifications without notice.

END OF SECTION