Author: aeghbal aeghbal
Last saved by: ali

DIVISION 27 21 29
Vi30103 L2 Drop and Insert 3-Port 60W PoE Switch
PART 1 - GENERAL
1.1	SUMMARY
A.	L2 Drop and Insert 3-Port 60W PoE Switch

1.2	SECTION INCLUDES
A.	Vi30103 L2 Drop and Insert 3-Port 60W PoE Switch

1.3	REFERENCES
A.	CE - European Union Compliance (CE)
B.	RoHS - Restriction of Use of Hazardous Substances
C.	WEEE - Waste Electrical and Electronic Equipment Directive
D.	RFC - Request for Comments
E.	IEEE - Institute of Electrical and Electronics Engineers
F.	EN/IEC - International Electrotechnical Commission

1.4	SYSTEM DESCRIPTION
B.	Connection Requirements: Provide three RJ45 connections:
1.	The system shall utilize a Category 5/5e/6 cables terminated in an RJ45 connector with EIA568-B configuration for PoE and data in for standard 10Base-T or 100Base-T for network transmission ports.
2.	The system shall utilize a Category 5/5e/6 cables terminated in two RJ45 connector with EIA568-B configuration for PoE and data out for standard 10Base-T or 100Base-T for drop and insert ports.

1.5	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed Installation and Operating Instruction
B.	Warranty: Manufacturer’s Printed Warranty

1.6	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate-controlled environment.
B.	Storage temperature not to exceed: -40˚C to +85˚C.

1.7	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of -20˚C to +60˚C without the assistance of forced-air cooling.
B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 95% (non-condensing). 

1.8	WARRANTY
A.	Limited Lifetime Warranty: Vigitron guarantees product to be free of defects for product’s lifetime, defined as the time that product is in production plus 3 years from the end of production.

1.	1
2.	2

PART 2 - PRODUCTS
2.1	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc. 7810 Trade Street, Suite 100, San Diego, CA 92129, USA 
2.	Phone: 1-858-484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted

2.2	MANUFACTURED UNITS
A.	Reference Table A: Product Number, Descriptions and Maximum Distance
B.	Reference Table B: IEEE Product Compatibility Chart
C.	Reference Table C: Product System Compatibility Chart

2.3	GENERAL SPECIFICATIONS
A.	The Drop and Insert 3-Port Switch shall be the Vi30103.
B.	Ethernet Ports:
1.	The Device shall support the Ethernet data IEEE 802.3/802.3u and 10/100Base-TX protocol.
2.	Data rate shall be automatically detected.
3.	The Device shall process Jumbo Frame packets up to 1,552 bytes at all speeds.
4.	The Device features two fixed 10/100TX electrical ports in a compact mini chassis.
a.	The Ethernet port shall comply with:
I.	IEEE 802.3 10Base-T 
II.	IEEE 802.3u 100Base-T 
5.	Ports shall be compliant to IEC 60603-7.
6.	The Device shall support standard Ethernet UTP connection distances up to 328 feet (100m) for all connections.
7.	The Device shall use Pass-Through PoE (PTP™) for PoE functions.
C.	The Device shall maintain all 802.3 PoE safety standards for PSE and PD communications.
D.	The Device shall have the ability to be powered by an 802.3af/at/bt (60W) PoE sources or an external 52-57VDC power source and provide 802.3 af/at PoE up to 30W per port on drop/repeater outputs.
E.	PoE levels are automatically sensed with no programming required.
F.	When connected in series, at any point, a qualified external power supply can be connected to boost the total PoE power output to 30W per port from that point.
G.	The Device shall consume less than 2.0W. 
H.	The Device shall provide LED indicators for monitoring proper system operation.
1.	Network LED Status:  
a.	Off – No Traffic
b.	Flashing – Traffic Present
2.	PoE: On- PoE power available

2.4	DATA SPECIFICATIONS
A.	Data Interface: Passage of data compliant to: 
1.	RFC 768 UDP
2.	RFC 2068 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 1783 TFTP
6.	RFC 894 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Data Rate: 10/100Mbps
C.	Data Connections: 3
1.	Three RJ45 connectors conforming to IEC 60603-7

2.5	The Vi30103 SPECIFICATIONS and FEATURE SETS
A.	The Device shall be able to perform as the following: 
B.	Packet losses per Device shall be less than one percent (1%) at 1,518 bytes.
C.	Packets per second (PPS) loss per Device shall be less than 1%.
D.	The Device shall process Jumbo Frames wire speed performance up to 10,000 bytes.
E.	The Device shall be able to connect and provide access up to nine (9) individual IP device addresses.
F.	The Device shall function as a fixed Layer 2 network switch with the following features:
1.	MDI-MDIX support
2.	IP DiffServ
3.	Port based QoS
4.	Broadcast Storm Protection
G.	The device must have the ability to be powered by IEEE 802.3af/at/bt (60W) compatible PoE.
I.	Vi30103 must have the Pass-Through-PoE (PTP^TM) functionality in compliance to IEEE 802.3af/at standards and non-standards 60W when communicating to a PD.
J.	The Device must have the ability to operate in extended temperature environments of -20˚C to 60˚C.
K.	The Device must provide the ability to display transmission connection continuity and data rate by means of LED indicators.

2.6	CONNECTORS
A.	Standard RJ45 connectors conforming to IEC 60603-7  

2.7	ELECTRICAL SPECIFICATIONS
A.	Power consumption: 2W
B.	PoE Input: IEEE 802.3af/at/bt up to 60W
C.	PoE Output: IEEE 802.3af/at (30W)
D.	Local Power supply Input: 48-57VDC up to 60W

2.8	MECHANICAL SPECIFICATIONS
A.	Dimensions: 0.97 x 1.76 x 2.7in, 2.5 x 4.5 x 6.9cm (HxWxL) 
B.	Finish: Extruded Aluminum
C.	Weight: 0.19lb, 177g

2.9	ENVIRONMENTAL SPECIFICATIONS 
A.	Operating Temp: -20˚C to +60˚C 
B.	Storage Temp: -40˚C to +85˚C
C.	Relative Humidity: 0% to 95% (Non-condensing)

2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS 
A.	FCC Part 15, Subpart B, Class B 2010  
B.	Emission Standards:
1.	EN 55022:206+A1:2007
2.	EN61000-3-2:2006+A1:2009+A2:2009
3.	EN 61000-3-3:2008
4.	EN55024:1998+A1:2001+A2:2003
C.	RoHS
D.	CE
E.	WEEE

2.11	MANUFACTURED UNITS REFERENCE TABLES

Table A: Product Number Descriptions
PRODUCT | DESCRIPTION | MAX. DISTANCE*
Vi30103 | Drop and Insert 60W PoE 3-Port Switch | 328 Feet (100m) @ 100Base-T
*Distance and performance figures are obtained using in house testing mirroring installation. Factors such as cabling, connections, use of power and environmental conditions may affect actual distance and should be taken in consideration. Distance represents single Device link.

Table B: Product IEEE Compatibility Chart
PRODUCT | | COMPATIBLE IEEE STANDARDS

Vi30103

IEEE 802.3u     IEEE 802.3af      
IEEE 802.3at
IEEE 802.3bt

Fast Ethernet standard for 10/100TX
Power over Ethernet output
Power over Ethernet
Power over Ethernet up to 60W (input only)

Vigitron reserves the right to change products or specifications without notice.

END OF SECTION