Title: Vi3026 A&E
Subject: High Power PoE Network Switch
Author: mngo
Last saved by: ali
Company: Hewlett-Packard Company

DIVISION 27 21 29
Vi3326 26-port Gigabit Ethernet L2 Plus Managed PoE Switch 
PART 1 - GENERAL
1.1	SUMMARY
A.	26-port Gigabit Ethernet L2 Plus Managed PoE Switch

1.2	SECTION INCLUDES
A.	Vi3326 26-port Gigabit Ethernet L2 Plus Managed PoE Switch

1.3	REFERENCES
A.	European Union Compliance (CE)
B.	Rohs
C.	WEEE compliant 
D.	UL – Underwriters Laboratory 
E.	FCC
F.	CE

1.4	SYSTEM DESCRIPTION
A.	Performance Requirements: Provides 26 ports for network switching.
B.	The system shall utilize TIA/EIA 568-B cable connected to an RJ-45 plug. 
C.	The system shall utilize sockets conforming to the Multiple Source Agreement INF 8074i.

1.5	SUBMITTALS
A.	Manufacturer’s Installation and Operational Manual: Printed Installation and Operational Information
B.	Warranty: Manufacturer’s Printed Warranty
C.	CLI

1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store in original packaging in a climate controlled environment. 
B.	Storage temperature not to exceed: -20˚C to +70˚C.

1.7	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of 0˚C to +40˚C by using internal component fans.
B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 90% (non-condensing). 

1.8	WARRANTY
A.	Limited Lifetime Warranty: Vigitron guarantees product to be free of defects for the product lifetime, defined as the time that product is in production plus 3 years from the end of production.

PART 2 - PRODUCTS
2.01	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc. 7810 Trade Street, Suite 100, San Diego, CA 92121, USA 
2.	Phone 1-858-484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted

2.02	MANUFACTURED UNITS
A.	Reference Table A: Compatible ANSI/IEEE Standards 
B.	Reference Table B: Compatible Ethernet Equipment

2.03	GENERAL SPECIFICATIONS
A.	The switch shall contain 26 active ports. 
B.	All ports be user programmable for port speeds of 10, 100, and 1000Mbps.
C.	All ports shall support Jumbo Frames at port speeds of 100Mbps and 1000Mbps. 
D.	The switch shall support internal bandwidth up to 52Gbps.
E.	The switch shall support a through-put of 95.232Mbps.
F.	Four ports 21, 22, 23, and 24 shall be shared with SFP sockets. 
1.	Use of these sockets with SFP shall disable the corresponding RJ-45 connector.
G.	The switch shall have two ports, 25 and 26, reserved for up and downlinks using SFP.
H.	The switch shall allow SFP for the use of SFP modules, conforming to the Multiple Source Agreement. This allow for flexibility in the determination of wavelength, range, type of receptacle, and type of fiber used. 
I.	The switch shall be compliant to IPv4 and IPv6.
J.	The switch shall be model Vi3326.
K.	Standard Ethernet Ports:
1.	The device shall have 24 standard Ethernet ports and 6 SFP ports in a compact housing. The Ethernet port shall comply with: 
a.	IEEE 802.3u 10baseT 
b.	IEEE 802.3u 100baseT 
c.	IEEE 802.3ab 1000baseT
2.	The SFP ports 21, 22, 23, and 24 shall comply with: 
a.	IEEE 802.3u 10baseT 
b.	IEEE 802.3u 100baseT 
c.	IEEE 802.3ab 1000baseT
3.	SFP Ports 25 and 26 shall comply with: 
a.	IEEE 802.3ab 1000baseT
4.	The standard ports of device shall support Standard Ethernet UTP connection distances up to 100m.
L.	Port bandwidth settings shall be done by automatic detection or manual selection.
. 

2.04	DATA SPECIFICATIONS
A.	Data Interface: Passage of data compliant to -
1.	RFC 768 UDP
2.	RFC 2068 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 1783 TFTP
6.	RFC 894 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Port Data Rate: 10/100/1000 Mbps
C.	Data Connections: 
1.	24 Standard Ethernet ports
2.	6 MSA compliant SFP sockets 

2.05	SPECIFICATIONS AND FEATURE SETS
A.	The Vi3326 transmits and receives data. 
1.	Internal bandwidth shall be constant with no more than a 2% decrease, when the input signal varies from a size of 64 bytes to 4500 bytes using bidirectional transmission and 9600 bytes unidirectional.
2.	Internal bandwidth shall be constant over the quoted extended distance with no more than 2% decrease when: 
a.	Bidirectional signals are transmitted with a packet size of 4,500 bytes.
b.	Unidirectional signals are transmitted with a packet size of 9,600 bytes.
c.	Bandwidth shall remain the same for both upload and download operation.
B.	Packet losses shall be at 2% or less at packet sizes, ranging from 64 bytes to 4,500 bytes bidirectional and 9,600 bytes unidirectional at both 100Mbps and 1000Mbps.
C.	Packets per second (PPS) shall not vary more than 2% at packet sizes, ranging from 64 bytes to 4,500 bytes for bidirectional transmission and 9,600 bytes for unidirectional at both 100Mbps and 1000Mbps.
D.	Maximum distance from switch port to device shall be 100m/328ft for data.
E.	The switch shall have the ability to detect all connected devices to individual ports or programmed to VLANs, and display them via GUI. 
F.	The switch shall contain an individual port “Easy Port” set-up, allowing for automatic programming for all ports set up for either IP Cameras or VoIP telephone systems. 
G.	The switch shall have a virtual stacking feature, to allow access to network switches located on the network, regardless of location, by accessing a single master switch IP address.
1.	 Master switch shall have the ability to control and obtain information from 31 additional switches. 
2.	 In virtual stacking mode switch shall have the ability to access devices on networks with different subnets
H.	The switch shall provide for multicasting via IGMP Querier and IGMP v1/v2/v3. It shall provide multicast traffic only to requesting network devices, in addition to source-specific multicasting. 
I.	The switch shall provide for Standard Spanning Tree (802.1d), Rapid spanning Tree-RSTP (802.1w), and Multiple Spanning Tree-MSTP (802.1s).
J.	The switch shall provide Private VLAN Edge isolation between clients in the same VLAN, supporting multiple uplinks. 
K.	The switch shall provide the ability to lock specific MAC addresses to specific ports, while user programming shall provide the ability to limit the number of allowed MAC addresses per port. 
L.	The switch shall provide individual IP port protection to prevent illegal IP addresses access to specific ports as per user programming. 
M.	The switch shall support SNMP Version 1, 2c, and 3, the later with user based security models (USM) and support for common traps. 
N.	The switch shall allow for firmware upgrades via HTTP/HTTPs and TFTP, in addition to directly via an on board console port.
O.	The switch shall allow for secure in band management using SSH/SSL, Telnet, SNMP and HTTP.
P.	Switch shall have the ability to create VLANS across multiple different switches in the same network. 

Q.	The switch shall support Microsoft ™ Internet Explorer version 6 or later, and Mozilla Firefox version 2.5 or later, operating on Microsoft Windows™, Linux, and Mac OS X.  

2.06	CONNECTORS
A.	Power In-let 
B.	Console Port 
C.	Standard Ethernet: RJ-45, IEC 60603-7
D.	SFP Port: MSA Compliant 

2.07	ELECTRICAL SPECIFICATIONS
A.	Power Supply:Input 100-240 VAC, 50/60Hz, Auto-sensing

2.08	MECHANICAL SPECIFICATIONS
A.	Dimensions (H x W x L): 1.75x17x12 in (4.3x43x30.5 cm)
B.	Finish: Device shall be constructed of a metal enclosure. 
C.	Weight: 11.2 pounds/ 5.1kg

2.09	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temperature: 0˚C to +40˚C
B.	Storage Temperature: -20˚C to +70˚C
C.	Relative Humidity: 10% to 90% (non-condensing)

2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS
A.	FCC Part 15, Subpart A
B.	Emission Standards: 
1.	FCC Part 15, Subpart B, Class A
2.	EN 55022:206+A1:2007
3.	EN61000-3-2:2006+A1:2009+A2:2009
4.	EN 61000-3-3:2008
5.	EN55024:1998+A1:2001+A2:2003
C.	Safety:
1.	CSA C22.2 NO. 60950-1-07-CAN/CSA INFORMATION TECHNOLOGY EQUIPMENT SAFETY PART GENERAL REQUIREMENTS - Edition 2 - Revision Date 2011/12/19 - Pending
2.	UL 60950-1 INFORMATION TECHNOLOGY EQUIPMENT - SAFETY - PART 1: GENERAL REQUIREMENTS - Edition 2 - Revision Date 2014/05/13 - Pending
D.	RoHS
E.	CE

2.11	MTBF
A.	The MTBF shall be >204,000 hours when operated at +25˚C/+77˚F.
B.	The MTBF shall be >116,000 when operated at +40˚C/+104˚F.
C.	The testing method shall be Telcordia Issus 1.

2.12	STANDARD ACCESSORIES
A.	AC Power Cord  
B.	Rack Mount Brackets with Screws
C.	RS 232 Console Cable 
D.	Information Disc: 
1.	Operations Manual 
2.	CLI Document 
3.	Quick Install Guide 
4.	Quick Set-up Guide

2.13	MANUFACTURED UNITS REFERENCE TABLES

PRODUCT | | IEEE/ANSI STANDARDS

802.3
802.3u   
802.3ab   
802.3z
Auto –negotiation 
IEEE 802.3x
IEEE 802.1q
IEEE 802.1p
IEEE 802.1x
IEEE 802.1d
IEEE 802.1w
IEEE 802.1s
IEEE 802.1ad
IEEE 802.1AB
IEEE 802.3az
IEEE 802.3ad
IEEE 802.1Q

ANSI/IEEE 802.3
Ethernet 10baseT UTP
Fast Ethernet 1000baseTX UTP 
Ethernet 1000baseTX UTP 
Ethernet 1000baseX 
Flow control Capability 
VLAN
Class of Service 
Access Control 
Spanning Tree
Rapid Spanning Tree 
Multiple Spanning Tree
Link Aggregation Control Protocol (LACP)
Link Layer Discovery Protocol (LLDP) 
Energy Efficient Ethernet Task
Trunking 
Tag Based VLAN

Table A: Compatible ANSI/ IEEE Standards

PRODUCT | COMPATIBLE ETHERNET EQUIPMENT

Vi3326

The device is compliant to standard IP Ethernet protocols 
The device is compliant to Link Layer Discovery Protocol (LLDP-IEEE 802.1AB with LLDP-MED extensions 
The device is compliant to UPnP Protocal

Table B. Compatible Ethernet Equipment 

	

Vigitron reserves the right to change products or specifications without notice.

END OF SECTION