Author: mngo
Last saved by: ali
Company: Hewlett-Packard Company

DIVISION 27 21 29
Vi3202 Coax Ethernet Extender w/60W PoE & DC input
PART 1 - GENERAL
1.01	SUMMARY
A.	Coax Ethernet Extender w/60W PoE & DC input 

1.02	SECTION INCLUDES
A.	Vi3202  Coax Ethernet Extender w/60W PoE & DC input 

1.03	REFERENCES
A.	CE - European Union Compliance (CE)
B.	RoHS - Restriction of Use of Hazardous Substances
C.	WEEE - Waste Electrical and Electronic Equipment Directive
D.	UL, cUL - Underwriters Laboratory
E.	RFC - Request for Comments
F.	IEEE - Institute of Electrical and Electronics Engineers
G.	EN/IEC - International Electrotechnical Commission

1.04	SYSTEM DESCRIPTION
A.	Performance Requirements: Provide 1 Ethernet extended distance 10/100BaseT port and 1 10/100Base-TX standard port providing data and PoE.
B.	The system shall utilize TIA/EIA 568-B cable connected to an RJ45 plug for standard Ethernet.
C.	The system shall utilize a BNC 1978 standard IEC 169-8 connector for extended transmission.

1.05	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed installation and operating information
B.	Warranty: Manufacturer’s Printed Warranty

1.06	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate controlled environment. 
B.	Storage Temperature not to exceed: -40˚C to +85˚C

1.07	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of -40°C to +75°C without the assistance of fan-forced cooling.
B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 90% (non-condensing). 

1.08	WARRANTY
A.	Limited Life Time Warranty: Vigitron guarantees product to be free of defects for product lifetime, defined as the time that product is in production plus 3 years from end of production.

PART 2: PRODUCTS

2.1	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc. 7810 Trade Street, Suite 100, San Diego, CA 92121, USA 
2.	Phone 1-858-484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted

2.2	MANUFACTURED UNITS
A.	Reference Table A: Product Number, Descriptions and Maximum Distance
B.	Reference Table B: IEEE Product Compatibility Chart

2.3	GENERAL SPECIFICATIONS
A.	The 12VDC/24VAC input Coax Ethernet 60W PoE Midspan Extender shall be the Vi3202.
B.	Standard Ethernet Ports:
1.	The device shall have one 10/100BaseT standard Ethernet ports in a compact housing:
a.	The Ethernet port shall comply with: 
i.	IEEE 802.3u 10baseT 
ii.	IEEE 802.3u 100baseT 
2.	The standard ports shall be compliant to IEC 60603-7.
3.	The device shall support Standard Ethernet UTP connection distances up to 100 meters.
4.	The device shall be compliant to IEEE 802.3af and IEEE 802.3at Type 1 and 2 standards and 60W UPoE compliant 60W.
5.	The Bandwidth selection shall be done by automatic detection.
6.	The device shall be used as either transmitter or receiver in the same system.
C.	The Extended Distance Ethernet Ports:
1.	Shall support distances up to 5,000 ft. (1,524m) at 10BaseT. 
2.	Shall support distances up to 2,000 ft. (606m) at 100BaseT. 
3.	Shall support the ability to pass standard IP Ethernet communications from a source to a device at the stated distances. 
4.	The extended coax port shall support 10/100BaseT at following distances:
a.	10Mbps at 5,000 ft. (1,515m)
b.	100Mbps at 2,000 ft. (606m) 
5.	Shall maintain all IEEE 802.3af/at safety standards for PSE and PD communications. 
6.	Shall maintain all IEEE 802.3 safety standards for up to 60W.
D.	The system shall provide the ability to test and verify connection status and operating bandwidth between two transceivers over the extended connection.
E.	The device shall be powered by a 24VDC, 24VAC 6 amps source.
1.	Power shall provide by a two wire terminal block.
F.	Unit shall consume less than 4W of power.
G.	The device shall provide below LED indicators for monitoring proper system operation: 
1.	Power: Red indicates power on
2.	Extended distance traffic/Link: Orange
a.	Off: No traffic
b.	Flashing: Traffic
3.	Extended Bandwidth indication:
a.	10BaseT: Green indicating 10BaseT
b.	100BaseT: Orange indicating 100BaseT
4.	Standard Ethernet Connections: Green
a.	Off indicating no connection 
b.	Flashing: connection with traffic
5.	Standard Ethernet Bandwidth indication
a.	10/100BaseT Yellow
b.	Off: no connection 
c.	On: connection is valid
H.	The unit shall automatically sense the optimum bandwidth and adjust accordingly.

2.4	DATA SPECIFICATIONS
A.	Data Interface: Passage of data compliant to: 
1.	RFC 768 UDP
2.	RFC 2068 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 1783 TFTP
6.	RFC 894 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Data Rate: 10/100 Mbps
C.	Data Connections: 1 standard Ethernet ports and 1 extended coax ports

2.5	Vi3202 FEATURE SETS
A.	Extender shall be able to accept a power source of 24VAC or 24VDC at 6 A and provide a PoE output compatible to the IEEE 802.3 PoE standards at: 
1.	IEEE 802.3af, Classes 0,1,2,3
2.	IEEE 802.3at Class 4 
3.	The 60W PoE shall be compatible with IEEE 802.3 PoE transmission and safety standards. 
B.	The extender device shall transmit and receive data using Symmetric Bandwidth (SBW™). 
1.	Bandwidth shall be constant over the quoted extended distance with no more than a 5% decrease, when the input signal varies from a size of 64 bytes to 4,500 bytes using bidirectional transmission.
2.	Bandwidth shall be constant over the quoted extended distance with no more than 5% decrease when: 
a.	Bidirectional signals are transmitted with a packet size of 4,500 bytes.
b.	Unidirectional signals are transmitted with a packet size of 9,000 bytes.
c.	Bandwidth shall remain the same for both upload and download operation.
C.	Packet losses shall be at 2% or less at packet sizes, ranging from 64 bytes to 4500 bytes bidirectional and 9,000 bytes unidirectional.
D.	Packet losses shall be at 2% or less at packet sizes of 4,500 in bidirectional transmission.
E.	Packets per second (PPS) shall not vary more than 5% at packet sizes, ranging from 64 bytes to 4,500 bytes.
F.	Packet per second (PPS) shall not vary more than 5% at packet of 4,500 bytes in bidirectional transmission.
G.	Maximum distance shall be 5,000 ft. (1,524m) at 10BaseT. 
H.	Maximum distance shall be 2,000 ft. (548m) at 100BaseT. 
I.	Extender device must have the ability to function as a Midspan. 
J.	Extender device must have the ability to be powered using 24VDC and 24VAC requiring 6 amps
K.	Extender shall have the ability to provide:
1.	IEEE 802.3af Class 3 PoE 
2.	IEEE 802.3at Class 4 PoE
3.	UPoE up to 60W
L.	Extender device must have the ability to operate as single PoE source, providing power to both transceivers and PD device conforming to IEEE 802.3af/at standards. 
M.	Extender device must have the ability to pass through PoE functionality in compliance with IEEE 802.3af/at standards when communicating with a PD: 
1.	Respond to detection pulses from PSE to PD.
2.	Respond to classification pulses from PSE to PD.
3.	Respond to required power from PSE to PD. 
4.	Ability to provide Class 2 IEEE 802.3af at maximum extended distance to both transceivers and PD from a PoE source. 
5.	Ability to provide Class 0, 1, 2, 3 and 4 IEEE 802.3af/at power to both compliant PD devices.
N.	Extender must be able to operate in extended temperature environments of -40°C to +75°C  
O.	Extender must provide the ability to test extended distance connection continuity and bandwidth by means of LED indicators. 

2.6	CONNECTORS
A.	Power: Pluggable 2 Pin connector 
B.	Extended Transmission Port: BNC 1978 standard, IEC 169-8
C.	Ethernet Port: RJ-45 : IEC 60603-7

2.7	ELECTRICAL SPECIFICATIONS
A.	Power Inputs
1.	12VDC  @  6A  
2.	24 VAC  @  3A 
3.	Power consumption 4W 

2.8	MECHANICAL SPECIFICATIONS
A.	Surface Mount Dimensions 5.62 x 2.4 x 1.9 in., 14.27 x 6.1 x 4.83 cm (HxWxL)
B.	Finish: Extruded Aluminum
C.	Weight 1.03lb, 466 g

2.9	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temp: -40°C to +75°C  
B.	Storage Temp: -40°C to +85°C 
C.	Relative Humidity: 0% to 95% (non-condensing)

2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS
A.	FCC Part 15, Subpart B, Class B 2010
B.	Emission Standards: 
1.	FCC Part 15, Subpart B, Class B 2010
2.	EN 55022:206+A1:2007
3.	EN61000-3-2:2006+A1:2009+A2:2009
4.	EN 61000-3-3:2008
5.	EN55024:1998+A1:2001+A2:2003
D.	RoHS
E.	CE

2.11	ACCESSORIES
A.	Operation Manual
B.	2-pin Terminal block to round connector adapter 

2.12	MANUFACTURED UNITS REFERENCE TABLES

PRODUCT | DESCRIPTION | MAX. DISTANCE*

Vi3202

Coax Ethernet Extender w/60W PoE & DC input

Extended Coax
5,000 ft. (1,524m) @ 10BaseT
2,000 ft. (606m) @ 100BaseT
Standard Ethernet 
328 ft. (100m) @ 100BaseT

Table A: Product Number Descriptions
*Distance and performance figures are obtained using in-house testing mirroring typical installations. Factors such as cabling, connections, use of power and environmental conditions may affect actual distance, and should be taken in consideration.

PRODUCT | | COMPATIBLE IEEE STANDARDS

Vi3202

IEEE 802.3u     IEEE 802.3af      
IEEE 802.3at

Fast Ethernet standard for 10/100TX
Power over Ethernet up to 15.4W
Power over Ethernet up to 30W

Table B: Product IEEE Compatibility Chart 

Vigitron reserves the right to change products or specifications without notice

END OF SECTION