Title: Vi2401 A&E specifications
Author: Neil Heller
Last saved by: aeghbal aeghbal
Company: HP

DIVISION 27 21 29
Vi50000A 1000Base-FX – 10/1000Base-TX Ethernet Fiber Media PoE Convertor with Built in PSE 
PART 1 - GENERAL
1.01	SUMMARY
A.	Vigitron Vi50000A is a fiber to copper media convertor with built-in PSE.
1.02	SECTION INCLUDES
A.	Vigitron Vi50000A 100/1000Base-TX Ethernet PSE-PoE Media Convertor MM/SM compatible up to 80km, depending on the SFP used.
1.03	REFERENCES
A.	CE - European Union Compliance (CE)
B.	RoHS – Restriction of Use of Hazardous Substances
C.	WEEE – Waste Electrical and Electronic Equipment Directive
D.	RFC - Request for Comments 
E.	IEEE - Institute of Electrical and Electronics Engineers
F.	EN/IEC - International Electrotechnical Commission
1.04	SYSTEM DESCRIPTION
A.	The Vi50000A will function as a layer 2 network switch providing PoE up to 65W. 
1.05	Performance Requirements 
A.	Performance Requirements: (1) 100/1000Base-Tx copper port with IEEE 802.3af (15.4W) / IEEE 802.3at (30W) compliant Power over Ethernet (PoE) Power Source (PSE) and 100/1000Base-FX, conforming to IEEE Transmission and PoE safety standards. 
1.	The system shall utilize a Small Format Pluggable (SFP) socket that conforms to the Multi Standards Agreement (MSA).
a.	The Vi50000A will be able to accept all forms of SFPs which conform to the MSA standards. 
2.	The system shall utilize EIA568, category 5/5e/6, 4-pair cables for 10Base-T, 100Base-TX or 1000Base-Tx to provide up to 30W PoE compliant to 802.3 PoE standards.
3.	Supports Jumbo Frames up to 9,000 bytes.
4.	The device will be able to accept power from a DC power source, ranging from 12VDC or 57VDC depending upon the required power output:
a.	12VDC @ greater than 2W will be used to power the Vi50000A, when no PoE is required. 
b.	56VDC @ at 70W will be used to power the Vi50000A and provide 802.3af, at, bt up to 65W PoE to an external device. 

1.06	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed installation and operating information.
B.	Warranty: Manufacturer’s Printed Warranty
1.07	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate-controlled environment. 
B.	Storage temperature not to exceed: -40˚C to +85˚C 
1.08	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of -40˚C to +80˚C without the assistance of fan-forced cooling.
B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0˚C to 95˚C (non-condensing). 
1.09	WARRANTY
A.	Vigitron Return and Warranty Policy: Vigitron warrants the product to be free of factory defects for the production lifetime of the product plus 3 years.

PART 2 - PRODUCTS
2.01	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc.: 7810 Trade St., Suite 100, San Diego, CA 92121, USA 
2.	Phone: +1 (858) 484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted
2.02	MANUFACTURED UNITS
A.	Model Number Descriptions: Reference Table A: Product Number Descriptions 
B.	Model Compatibility Chart: Reference Table B: Product Compatibility Chart
C.	Optional Accessories: Reference Table C: Optional Accessories Chart 
2.03	GENERAL SPECIFICATIONS
A.	The 100/1000Base-TX PoE media convertor to Fiber SFP shall be Vigitron Vi50000A. 
B.	The Vi50000A shall comply with MSA standards for SFP.
C.	The Vi50000A shall provide bidirectional media conversion between fiber and copper.
D.	The Vi50000A shall support the following standards:
1.	Ethernet data IEEE 802.3/802.3u 10/100Base-TX and 1000BaseT, 802.3z protocol using auto-negotiating and auto-MDI/MDI-X features.
2.	Fiber PHY conforming to 100Base and 1000Base-FX.
E.	The Vi50000A shall have the following performance:
1.	Support for flow control for full duplex (symmetric/asymmetric) and half duplex (collision/carrier base) operation
2.	9K jumbo frame packet transmission
F.	The Vi50000A shall also inject power by transmitting DC voltage to the Cat 5/5e cable, and transfer data and power simultaneously to PoE Powered Device.
G.	The Vi50000A shall detect PoE IEEE 802.3af, 802.3at PD, and dual PD devices up to 30W equipment automatically, and protect devices from being damaged by incorrect installation.
H.	The Vi50000A shall support UTP distance up to 100m.
I.	The Vi50000A shall support the transmission of up to 1000Mbps over a single mode or multimode fiber, depending upon the SFP used.
J.	The Vi50000A shall provide power, fiber port status, copper port status, and PoE in-use status to indicate the LEDs for monitoring proper system operation.
K.	The Vi50000A shall be able to:
1.	When there is no PoE output, it will accept a DC power source of 12VDC.
2.	Provide 802.3af PoE power, when a power source of greater than 17W at 48VDC is used.
3.	Provide 802.3at PoE power, when a power source of greater than 32W at 48VDC is used.
4.	Maximum PoE accepted power will be 70W at 56VDC.
2.04	Ethernet DATA SPECIFICATIONS
A.	Data Interface: Ethernet IEEE 802.3u 
B.	Data Interface: Ethernet IEEE 802.3z 
C.	Data Rate: 10/100/1000 Mbps
D.	Connection: One RJ45 connector
E.	Operation Mode: Full Duplex / Half Duplex
2.05	OPTICAL SPECIFICATIONS
A.	Vigitron Vi50000A
1.	Optical Fiber via SFP
2.	Number of Optical Ports: 1
3.	Optical Wavelength: 1310nm and 850nm
4.	Optical Power Budget: Depends on SFP
5.	Maximum Distance: Depends on SFP

2.06	STATUS INDICATORS
A.	System
LED | COLOR | FUNCTION
PWR | Green | On | Unit is powered.

B.	10/100Base-TX Port
LED | COLOR | FUNCTION
LINK/ACT | Orange | Blink | There is a link with activity.
| | On | There is a link to a connected device.
| | Off | There is no link.
Link Speed | Green | On | There is a 1G link to the connected device.
| | Off | There is not a 1G link.
PoE in Use | Green | On | PoE power is being delivered to the connected device.
| | Off | There is no PoE power being used.

C.	1000Base-SFP (This relates to function of main unit no SFP)
LED | COLOR | FUNCTION
LINK/ACT | Green | Blink | There is a 1G link with activity.
| | Lit | There is a 1G link but with no activity.
| | Off | There is no link.

2.07	CONNECTORS
A.	Power: 2-pin Terminal Block
B.	Optical: Via MSA Compliant SFP Socket
C.	Data over Cat5/5e/6: RJ-45 Connector
2.08	ELECTRICAL SPECIFICATIONS
A.	Power Input: 12VDC or 48VDC- 57VDC, Maximum power input 120W @ 56 volts
B.	The PoE Output: IEEE 802.3af, IEEE 802.3at or IEEE 802.3at IEEE 802.3bt (depending on the input power supply)
2.10	MECHANICAL SPECIFICATIONS
A.	Surface Mount Dimensions: 0.97 x 1.75 x 4.26in., 2.46x4.45x10.8 cm (HxWxL) 
B.	Finish: Module shall be constructed of a metal enclosure.
C.	Weight: 0.235 lbs (107g) 
2.10	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temp: -40°C to 80°C
B.	Storage Temp: -40°C to +85°C
C.	Relative Humidity: 0% to 95% (Non-condensing)
2.11	REGULATORY AGENCIES/APPROVALS AND LISTINGS 
A.	Federal Communications Commission (FCC) Part 15, Class A  
B.	European Union Compliance (CE) with the following standards:
1.	EN 55022:2006, Class A
2.	EN 61000-3-2:2006
3.	EN 61000-3-3+A2:2005
4.	EN 55024+A2:2003
C.	RoHS
D.	WEEE 
PART 3 - EXECUTION
3.01	PREPARATION
A.	Standalone Module (Surface Mount)
1.	Shall be mounted on a properly prepared surface adequate for the size and weight of the module. The placement of the unit shall allow provision for cable installation and maintenance as indicated on the approved detail drawings and in compliance with the installation manual.
B.	Optical Fibers
1.	Caution: NEVER look into the end of an active optical fiber when using a laser light output. Eye damage can occur. Wear eye protection when cleaning, terminating, and splicing the fiber.
2.	The number and type – Multimode / single mode of the optical fiber shall be the requirements of the selected SFP and used for both cable ends.
3.	All optical fiber cables shall be properly installed and terminated with the mating optical connectors.
4.	The optical connectors on the cable shall be cleaned in compliance to the optical connector manufacturer’s specifications and covered with dust caps until connection to the fiber optic module.

3.02	INSTALLATION
A.	General: The Vi50000A shall be installed in compliance with the Ethernet standards and is not to be more than 328 ft. (100m) away from the PoE powered device. 

3.03	MANUFACTURED UNITS REFERENCE TABLES

Vigitron Part No. | Description | Max. Distance*
Vi50000A | 100Base-TX to 1000Base Fiber Media Convertor with Built-in 802.3af, at, bt up to 65W | Up to 80Km depending on the type of SFP and fiber cabling used
Table A: Product Number Descriptions 
* Maximum distance is limited to optical loss of the fiber and any additional loss by connectors, splices, and patch panels.

Vigitron Part No. | Compatible Ethernet Equipment

Vi50000A

All products conform to:
1.	Use of SFP conforming to MSA standards
2.	Conforming to IEEE standards for Ethernet transmission
3.	Conforming to IEEE standards for 802.3af PoE
4.	Conforming to IEEE standards for 802.3at PoE
5.	Conforming to IEEE standards for 802.3bt PoE

Table B: Product Compatibility Chart

* Note: Optional Accessories are not required to operate the Vi50001. You may use other sources. However, Vigitron does not guarantee or warranty performance of products other than Vigitron labeled or provided.

Vigitron reserves the right to change products or specifications without notice.

END OF SECTION