Author: Neil Heller

DIVISION 27 21 29
Vi22001U Single Port 90W 802.3af/at/bt, PoE Midspan
PART 1 - GENERAL
1.01	SUMMARY
Single Port 90W 802.3af/at/bt, PoE Midspan 

1.02	SECTION INCLUDES
Vi22001U Single Port 90W 802.3af/at/bt, PoE Midspan

1.03	REFERENCES
A.	European Union Compliance (CE)
B.	RoHS 
C.	WEEE 
D.	UL - in progress

1.04	SYSTEM DESCRIPTION
A.	Performance Requirements: Single port Midspan providing up to 90W PoE power 
B.	The system shall utilize TIA/EIA 568-B cable connected to an RJ-45 plug
C.	The system shall utilize EIA568-B, Category 5/5e/6, 4-pair cables for 10/100/1000Base-T.

1.05	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed installation and operating information.
B.	Warranty: Manufacturer’s printed warranty.

1.06	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate-controlled environment. 
B.	Storage temperature not to exceed: -40˚C to +85˚C.

1.07	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with ambient temperature range of:
PoE Power Output | Ambient Temperature
90W | +45°C
75W | +50°C
60W | +55°C
37W | +60°C

B.	Shall have the ability to cold start at -20˚C.
C.	Overall operating temperature shall be -40˚C to 60˚C
D.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 95% (non-condensing). 

1.08	WARRANTY
A.	Limited Lifetime Warranty: Vigitron guarantees the product to be free of defects for the product lifetime, defined as the time that the product is in production or 3 years, whichever is longer.

PART 2 – PRODUCTS
2.01	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc.: 7810 Trade St., San Diego, CA 92121, USA 
2.	Phone: +1 (858) 484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted

2.02	MANUFACTURED UNITS
A.	Reference Table A: Product Number Descriptions and Maximum Distance 
B.	Reference Table B: IEEE Product Compatibility Chart
C.	Reference Table C: Product System Compatibility Chart 

2.03	GENERAL SPECIFICATIONS
A.	The product has two RJ-45 ports 
1.	  Data Port: shall comply with: 
a.	IEEE 802.3 10base-T 
b.	IEEE 802.3u 100base-T
c.	IEEE 802.3u 1000base-T.	
2.	  Data + PoE port: shall comply with: 
a.	IEEE 802.3af
b.	IEEE 802.3at 
c.	IEEE 802.3bt class 0-8 up to 90W
3.	  Standard ports shall be compliant to IEC 60603-7.
4.	  The device shall support standard Ethernet UTP connection distances up to 328 ft. (100m).
B.	The Vi22001U:
1.	Shall support the ability to provide IEEE 802.3af/at/bt up to 90W PoE power at the stated distances to a PD device.
2.	Shall maintain all IEEE 802.3af/at/bt safety standards.
3.	Shall provide for without the need for operational programing for: 
a.	Recognition of PD device
b.	Recognition of PD device class 
c.	LED Indicators
i.	Power on/off
ii.	PoE on/off

2.04	DATA SPECIFICATIONS
A.	Data Interface: Passage of data compliant to:
1.	RFC 768 UDP
2.	RFC 2068 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 1783 TFTP
6.	RFC 894 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Data Rate: 10/100/1000 Mbps
C.	Data ports: 
1.	RJ45 standard Ethernet ports 
D.	Data + PoE Port: 
1.	RJ45 standard Ethernet ports  
E.	PoE Power Outputs: 
1.	15.4W compliant to IEEE 802.3af 
2.	30W complaint to IEEE 802.3at Type 1 and Type 2
3.	90W compliant to IEEE 802.3bt, Compatible with single PD and dual PD devices
4.	Power output pins: 
a.	1 & 2 negative, 3 & 6 positive
b.	4 & 5 positive, 7 & 8 negative

2.05	SPECIFICATIONS AND FEATURE SETS 
A.	Must have the ability to:
1.	Recognition a standard a PD
2.	Recognize and respond to a PD class
3.	Ability to cease power in the event of a over current or other abnormal conditions at the load.

2.06	CONNECTORS
A.	Power: IEC380-8 Inlet 
B.	Ethernet: RJ-45 connector compliant to IEC 60603-7
C.	Ethernet and PoE: RJ-45: RJ-45 connector compliant to IEC 60603-7

2.07	ELECTRICAL SPECIFICATIONS
A.	Power Inputs:
1.	110-230VAC/50-60Hz, auto-sensing
B.	Output power: 
1.	90W @ 56-57VDC 

2.08	MECHANICAL SPECIFICATIONS
A.	Dimensions (L x W x H): 5.71 x 3.75 x 2 in., 15.5 x 9.5 x 5.1 cm 
B.	Finish: Extruded Aluminum 
C.	Weight: 1.58 lb. (720 g)
D.	Mounting: Table top and wall mount using side brackets 

2.09	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temp: -20˚C to +60 ˚C
B.	Cold Start: -20˚C
C.	Storage Temp: -40˚C to +85˚C
D.	Relative Humidity: 0% to 95% (Non-condensing)

2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS:
A.	CE
B.	RoHS Compliant 
C.	FCC Part 15, Subpart B, Class B 2010 (in progress) 
D.	Emission Standards: (in progress) 
1.	EN 55022:206+A1:2007
2.	EN61000-3-2:2006+A1:2009+A2:2009
3.	EN 61000-3-3:2008
4.	EN55024:1998+A1:2001+A2:2003

2.11	ACCESSORIES
A.	Operation Manual 
B.	IED 7ft. Power Cord
C.	Mounting brackets

2.12	MANUFACTURED UNITS REFERENCE TABLES

Product | Description | Max. Distance*
Vi22001U | Single port 90W Midspan | Depends on PD Power Requirement
Table A: Product Number Descriptions 
* Distance figures are obtained using in-house testing mirroring installation. Factors such as cabling, connections, use of power, and environmental conditions may affect the actual distance and should be taken in consideration.

Product | Compatible IEEE Standards

Vi22001U

IEEE 802.3u Ethernet standard for 10/100/1000TX protocol
IEEE 802.3af Power over Ethernet 
IEEE 802.3at Power over Ethernet
IEEE 802.3bt Power over Ethernet
.

Table B: Product IEEE Compatibility Chart

Vigitron reserves the right to change products or specifications without notice.

END OF SECTION