Author: Neil Heller

DIVISION 27 21 29
Vi22401U Single Port 60W IEEE 802.3bt Midspan
PART 1 - GENERAL
1.01	SUMMARY
A.	Single port 60W IEEE 802.3bt Midspan 
1.02	SECTION INCLUDES
A.	Vi22401U single port 60W IEEE 802.3bt Midspan 

1.03	REFERENCES
A.	European Union Compliance (CE)
B.	RoHS 
C.	WEEE 
1.04	SYSTEM DESCRIPTION
A.	Performance Requirements: Single port Midspan providing 60W PoE power 
B.	The system shall utilize TIA/EIA 568-B cable connected to an RJ-45 plug
C.	The system shall utilize EIA568-B, Category 5/5e/6, 4-pair cables for 10/100/1000Base-T.
1.05	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed installation and operating information.
B.	Warranty: Manufacturer’s printed warranty.
1.06	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate-controlled environment. 
B.	Storage temperature not to exceed: -40˚C to +85˚C.
1.07	PROJECT/SITE CONDITIONS
A.	Shall have the ability to cold start at -20˚C.
B.	Overall operating temperature shall be -20˚C to 50˚C
D.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 95% (non-condensing). 

1.08	WARRANTY
A.	Limited Lifetime Warranty: Vigitron guarantees the product to be free of defects for the product lifetime, defined as the time that the product is in production or 3 years, whichever is longer.

PART 2 – PRODUCTS
2.01	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc. 7810 Trade Street, Suite 100, San Diego, CA 92121, USA 
2.	Phone 1-858-484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted
2	MANUFACTURED UNITS
A.	Reference Table A: Product Number Descriptions and Maximum Distance 
B.	Reference Table B: IEEE Product Compatibility Chart
C.	Reference Table C: Product System Compatibility Chart 
2.03	GENERAL SPECIFICATIONS
A.	The product has two RJ-45 ports 
1.	Data Port: shall comply with: 
a.	IEEE 802.3 10base-T 
b.	IEEE 802.3u 100base-T
c.	IEEE 802.3u 1000base-T.	
2.	Data + PoE port: shall comply with: PoE Classes 0-6
a.	IEEE 802.3af
b.	IEEE 802.3at 
c.	IEEE 802.3bt up to 60W
3.	Standard ports shall be compliant to IEC 60603-7.
4.	The device shall support standard Ethernet UTP connection distances up to 328 ft. (100m).
5.	Shall support the ability to provide IEEE 802.3af/at/bt PoE power at the stated distances to a PD device.
6.	Shall maintain all IEEE 802.3af/at/bt safety standards.
7.	Shall provide for without the need for operational programing for: 
a.	Recognition of PD device
b.	Recognition of PD device class 
c.	LED Indicators
i.	Power on/off
ii.	PoE on/off
2.04	DATA SPECIFICATIONS
A.	Data Interface: Passage of data compliant to:
1.	RFC 768 UDP
2.	RFC 2068 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 1783 TFTP
6.	RFC 894 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Data Rate: 10/100/1000 Mbps
C.	Data ports: RJ45 standard Ethernet ports 
D.	Data + PoE Port: RJ45 standard Ethernet ports  
E.	PoE Power Outputs: Classes 0-6
1.	15.4W compliant to IEEE 802.3af 
2.	37W complaint to 802.3at Type 1 and Type 2
3.	60W IEEE 802.3bt, Compatible with single and dual PD devices. 
4.	Power output pins: 
a.	1 & 2 negative, 3 & 6 positive
b.	4 & 5 positive, 7 & 8 negative
2.05	SPECIFICATIONS AND FEATURE SETS 
A.	Must have the ability to:
1.	Recognition a standard a PD
2.	Recognize and respond to a PD class
3.	Ability to cease power in the event of an over current or other abnormal conditions at the load.

2.06	CONNECTORS
B.	Power: IEC-320-C14 Inlet 
C.	Ethernet: RJ-45 connector compliant to IEC 60603-7
D.	Ethernet and PoE: RJ-45: RJ-45 connector compliant to IEC 60603-7
2.07	ELECTRICAL SPECIFICATIONS
A.	Power Inputs:110-230VAC/50-60Hz, auto-sensing
B.	Output power: 60W @ 56-57VDC 
2.08	MECHANICAL SPECIFICATIONS
A.	Dimensions (L x W x H): 6.17 x 2.56 x 1.87 in., 15.3 x 6.5 x 4.7 cm 
B.	Finish: Extruded Aluminum 
C.	Weight: 0.95 lb (430 g)
D.	Mounting: Tabletop and wall mount using side brackets 
2.09	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temp: -20˚C to +50˚C
B.	Cold Start -20˚C
C.	Storage Temp: -40˚C to +85˚C
D.	Relative Humidity: 0% to 95% (Non-condensing)
2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS:
A.	CE
B.	RoHS Compliant 
C.	FCC Part 15, Subpart B, Class B 2010 (in progress) 
D.	Emission Standards: (in progress) 
1.	EN 55022:206+A1:2007
2.	EN61000-3-2:2006+A1:2009+A2:2009
3.	EN 61000-3-3:2008
4.	EN55024:1998+A1:2001+A2:2003
2.11	ACCESSORIES
A.	Operation Manual 
B.	IED 7ft. Power Cord

2.12	MANUFACTURED UNITS REFERENCE TABLES

Product | Description | Max. Distance*
Vi22401U | Single port 60W Midspan | Depends on PD Power Requirement
Table A: Product Number Descriptions 
* Distance figures are obtained using in-house testing mirroring installation. Factors such as cabling, connections, use of power, and environmental conditions may affect the actual distance and should be taken in consideration.

Specification | Compatible IEEE Standards

Ethernet
PoE
PoE
PoE

IEEE 802.3u Ethernet standard for 10/100/1000TX protocol
IEEE 802.3af Power over Ethernet 
IEEE 802.3at Power over Ethernet; Type 1 and Type 2 
IEEE 802.3bt Power over Ethernet, Class 0-6

Table B: Product IEEE Compatibility Chart

Product | Compatible Ethernet Equipment

Vi22401U

PoE powered products conforming to: 
IEEE 802.3af
IEEE 802.3at
IEEE 802.3bt

Table C: Product System Compatibility Chart

Vigitron reserves the right to change products or specifications without notice.

END OF SECTION