DIVISION 27 21 29
Vi22116U MaxiiPower™ 16-port Managed 802.3af/at/bt and High Power PoE Midspan
         Vi22108U MaxiiPower™ 8-port Managed 802.3af/at/bt and High Power PoE Midspan 
PART 1 - GENERAL
1.01	SUMMARY
A.	16-port 802.3af/at/bt  90W Managed PoE Midspan-Vi22116U
B.	8-port 902.3af/at/bt 90W Managed PoE Midspan-V22108U
C.	Note: Where model number is not indicated reference to both Vi22116U and Vi22108U 
1.02	REFERENCES
A.	European Union Compliance (CE)
B.	RoHS
C.	WEEE compliant 
D.	UL 
1.03	SYSTEM DESCRIPTION
A.	Performance Requirements: 
1.	Provide 16-ports of 802.3af/at/bt PoE power at 90W.-Vi22116U
2.	Provide 8- ports of 802.3af/at/bt PoE Power at 90W -Vi22108U
3.	Provide 16- ports of legacy High Power PoE to 74W .-Vi22116U
4.	Provide 8-ports of legacy High Power PoE to 74W-Vi22108U 
B.	The system shall utilize TIA/EIA 5616-B cable connected to an RJ-45 plug.
C.	The system shall utilize EIA5616-B, category 5/5e, 2-pair or 4-pair cables for 10Base-T/100Base-TX/1000-2500Tx baseT.
D.	Will provide 16- data only ports for connections to switches and like devices- Vi22116U
E.	Will provide 8-data only porta for connections to switches and like devices Vi22108U
1.04	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed Installation and Operating Information
B.	Warranty: Manufacturer’s Printed Warranty
1.05	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate-controlled environment. 
B.	Storage Temperature not to exceed: -30˚C to +70˚C
1.06	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of -10˚C to +40˚C without the assistance of fan-forced cooling.
B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 90% (non-condensing). 

1.07	WARRANTY
A.	Limited Lifetime Warranty: Vigitron warranties the product to be free of defects for the product’s lifetime, defined as the time product is in production plus 3 years.
PART 2 - PRODUCTS
2.01	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc. 7810 Trade Street, Suite 100, San Diego, CA 92121, USA 
2.	Phone 1-858-484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted
2.02	MANUFACTURED UNITS
A.	Reference Table A: Product Number Descriptions and Maximum Distance
B.	Reference Table B: IEEE Product Compatibility Chart
C.	Reference Table C: Product System Compatibility Chart
D.	Reference Table D: Redundant Power Supply Compatibility Chart
2.03	GENERAL SPECIFICATIONS
A.	The PoE Midspan shall be Vi22116U for 16 ports.
B.	The PoE Midspan shall be Vi22108U for 8 ports
C.	Ethernet Port:
5.	The module shall support the Ethernet data IEEE 1602.3/1602.3u 10/100Base-TX protocol.
6.	The Ethernet port will comply with: 
a.	IEEE 802.3 10baseT 
b.	IEEE 802.3u 100baseT 
c.	IEEE 802.3u 1000baseT
d.	IEEE 802.3bz 2500baseT
7.	Standard ports will be compliant to IEC 60603-7.
8.	The module shall support standard Ethernet UTP connection distances up to 100m.
D.	The Vi22116U/Vi22108U:
1.	Will support the ability to pass 802.3af/at/bt PoE from a source to a device at the stated distances providing PoE power to a PD device.
2.	Will provide up to 90W for at least 8 ports Class 0-8 Vi22116U/Vi22108U
3.	Will provide up to 74W for at least 9 ports for legacy high PoE-Vi22116U
4.	Will be able to power devices by using a single and dual PD.
5.	Will maintain all 802.3af/at/bt safety standards.
6.	Will provide programming for operational programing for: 
a.	Recognition of PD device
b.	Recognition of PD device class
c.	Recognition of individual port failure mode:
i.	Upon port failure, the LED will flash.  

E.	The Vi22116U/Vi22108U will provide operator management via web browser
F.	Software and user program will not be required for operation.
G.	Client software will provide enterprise level operation, allowing for set-up and monitoring over a network. 
H.	Unique MPoE™ operating system will provide immediate set up verification on a single web page 
I.	Connection by computer to Vi22116U/Vi22108U will be by means of:
1.	Over a network using standard Ethernet connections
J.	Software functions will include: 
1.	Programming functions: 
a.	Port Priority
b.	Port Enable 
c.	Port Disable 
d.	Force Power  
e.	Power Class 
f.	Autocheck Mode Operation
g.	Port Reset
h.	Port naming  
2.	Monitoring functions will include: 
a.	Port Status
b.	Allocated PoE power
c.	Total consumed PoE Power
d.	Total remaining PoE power 
e.	Port Consumption 
f.	Port Class 
g.	Port Status 
3.	Alarm monitoring functions:
a.	Via front panel LEDs.
b.	Monitoring via client software through: 
i.	On board GUI over network 
ii.	Syslog 
K.	The unit will deliver up on 90W per port with no power sharing for the  
L.	The Vi22116U shall deliver a per port maximum of 46W PoE when all ports are used to maximum
M.	The Vi22108U shall deliver a per port maximum of 90W PoE when all ports are used to maximum 
N.	Firmware will be upgradeable using the network connection port
M. The Vi22116U/Vi22108U will have the following LED indications: 
1. Front Panel
a. Power- LED on/LED off, Firmware upgrade-Flashing 
b. .Port-On Power delivering, Off no power 
   2. GUI 
	a. No PoE-Gray/blank-steady
	b. PoE Delivery- Green-steady
	c. Auto checking in process- Green steady delivering -Grey-steady off 
     d. Autochecking -failed – red -steady

2.04	DATA SPCIFICATIONS
A.	Data Interface: Passage of data compliant to -
1.	RFC 7616 UDP
2.	RFC 20616 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 17163 TFTP
6.	RFC 1694 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Data Rate: 10/100/1000Mbps
C.	Data Inputs: 
1.	16 standard Ethernet Ports 
2.05	Vi22116U/Vi22018U Specifications and Feature
A.	Maximum distance will be 328 ft. (100m) at all wire spe
B.	Must have the ability to provide full classes 0-8 802.3af/at/bt PoE for each port without power sharing between ports. 
C.	Must have the ability to provide up to 90W Classes 0-8 on all ports 
D.	Must have the ability to provide up 74W of legacy PoE on all pots 
E.	Must have the ability to recognize devices operating with single and dual PDs. 
F.	Must have the ability:
1.	Recognition of start-up PD voltage requirement.
2.	Recognize and respond to PD class.  
3.	Transmit and maintain power to PD. 
4.	Cease power transmission in the event of a shortage or other abnormal conditions. 
H.	Each port will be sampled for potential failure rate conditions. 
I.	Security will be provided via the use of a username and password 
J.	Client access shall be by known network browsers with username and password protection 
K.	The Midspan will have two Watchdogs:
1.		Input power in the form of voltage will be monitored. If voltage falls outside the range of 	42VDC to 59VDC power will shut down to protect the midspan and its connected 	devices.
2.		Internal communications, including the microprocessor, will be monitored every 15 	seconds. In the event of stalled or frozen communications the system will issue a reset 	restoring programming and operations 
2.06	CONNECTORS
A.	Power: IEC3160-16 Inlet 
B.	Standard Ethernet connector to be compliant to IEC 60603-7
C.	RJ45 network 
2.07	ELECTRICAL SPECIFICATIONS
A.	Power Inputs
1.	110-230V AC/ 50-60Hz @ 6.5A auto-sensing
B.	Output power: 
1.	56V DC @ 90W per port, 730W aggregated

2.08	MECHANICAL SPECIFICATIONS
A.	Surface Mount Dimensions (H x W x L):
1.	1.75 x 17 x 12 in (4.3 x 43 x 30.5 cm)
B.	Finish: Module shall be constructed of a metal enclosure.
C.	Weight:
1.	11lb, 5Kg
D.	Mounting: 
1.	Vi22116U/Vi22108U shall be able to be rack mount in a standard EIA 19” rack mount enclosure.
2.09	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temp: -10˚C to +40˚C
B.	Storage Temp: -30˚C to +70˚C
C.	Relative Humidity: 0% to 90% (non-condensing)
2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS
A.	CE
B.	RoHS 
C.	UL 60950-1, 2nd Edition, 2007-03-27, CSA C 22.2 No. 60950-1-07 2nd Edition, 2007-03
D.	FCC Part 15, Subpart B, Class B 2010
E.	Emission Standards: 
1.	EN 55022:206+A1:2007
2.	EN61000-3-2:2006+A1:2009+A2:2009
3.	EN 61000-3-3:20016
4.	EN55024:19916+A1:2001+A2:2003
F. Compliant: NDAA 
2.11	ACCESSORIES
A.	Operation Manual via download 
2.12	MANUFACTURED UNITS REFERENCE TABLES
Vi2200 Product Series	Description	Max. Distance*	
Vi22116U
Vi22108U	16-port  802.3af/at/bt PSE Midspan
8-port   802.3af/at/bt PSE Midspan 	328 ft. (100m) @ all wire speeds
328 ft (100) @ all wire speeds 
	
Table A: Product Number Descriptions 
* Distance figures are obtained using in-house testing mirroring installation. Factors such as cabling, connections, use of power and environmental conditions may affect actual distance and should be taken in consideration.

Extended Ethernet Transceiver 	Compatible IEEE Standards	
Vi22116U
Vi22108U
	IEEE 802.3u Fast Ethernet
IEEE 802.3af Power over Ethernet 
IEEE 802.3at Power over Ethernet
IEEE 802.3bt Power over Ethernet 
UPoE+ up to 72W	
Table B: Product IEEE Compatibility Chart

Extended Ethernet Transceiver	Compatible Ethernet Equipment	
Vi22116U
Vi22108U	Any device compliant to 802.3af/at/bt power inputs 	
Table C: Product System Compatibility Chart

Vigitron reserves the right to change products or specifications without notice.
END OF SECTION