# Vi30406U

P1

P2

P3

P4

SFP1

SFP2

Autochecking
Port 1:The IPv4 address of the device on port 1 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 2:The IPv4 address of the device on port 2 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 3:The IPv4 address of the device on port 3 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 4:The IPv4 address of the device on port 4 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port

Autochecking Setting
Duration (80 - 200s): Time between device checks |
Failed Threshold (3 - 7 Times): The number of failed tests before attemtping reboot |
Reboot Attempts (1 - 5 Times): The number of restart attempts before disabling power |