DIVISION 27 21 29
Vi30406U 5-port 1G PoE Powered PoE Network Switch
PART 1 - GENERAL
1.1	SUMMARY
A.	6-port 1G/2.5G UTP ports 1G/2.5G/10G Fiber ports  

1.2	SECTION INCLUDES
A.	Vi30406U 4 UTP-port 100/1000/2500Mbps+2 Fiber  1G/2.5G/10G Fiber Ports   

1.3	REFERENCES
A.	European Union Compliance (CE)
B.	Rohs
C.	WEEE Compliant 
D.	FCC
E.	CE

1.4	SYSTEM DESCRIPTION
A.	Performance Requirements: Provide 5 ports for network switching, one port can be used for powering the switch via PoE and four ports can be used for providing PoE to connected devices. 
1.	The system shall utilize TIA/EIA 568-B cable connected to RJ-45 plugs. 
2.	Two ports shall connect via fiber MSA compliant port 

1.5	SUBMITTALS
A.	Manufacturer’s Installation and Operating Manual: Printed Installation and Operating Information
B.	Warranty: Manufacturer’s Printed Warranty

1.6	DELIVERY, STORAGE AND HANDLING
A.	Store in original packaging in a climate-controlled environment. 
B.	Storage temperature not to exceed: -40˚C to +85˚C

1.7	PROJECT/SITE CONDITIONS
A.	Temperature Requirements: Product shall operate in an environment with an ambient temperature range of -40˚C to +70˚C subject to derating power.

B.	Humidity Requirements: Products shall operate in an environment with relative humidity of 0% to 90% (non-condensing). 

1.8	WARRANTY
A.	Limited Lifetime Warranty: Vigitron guarantees products to be free of defects for product lifetime, defined as the time that product is in production plus 3 years from end of production.

PART 2 - PRODUCTS
2.01	MANUFACTURER
A.	Acceptable Manufacturer: 
1.	Vigitron, Inc.: 7810 Trade Street Suite 100, San Diego, CA 92121, USA 
2.	Phone: +1 (858) 484-5209
3.	Email: support@vigitron.com
B.	Substitutions: Not Permitted

2.02	MANUFACTURED UNITS
A.	Reference Table A: Compatible ANSI/IEEE Standards 
B.	Reference Table B: Compatible Ethernet Equipment

2.03	GENERAL SPECIFICATIONS
A.	The switch shall contain 6 active ports. 4 UTP + 2 Fiber
B.	The switch shall be managed for: 
1.	Network integration via: 
a.	IP address assignment 
b.	PoE functions
C.	All Copper ports shall automatically detect network speeds of 100/1000/2500Mbps.
D.	All Fiber ports shall support network speeds of 1G/2.5G/10GMbps.  
E.	The switch shall support internal bandwidth up to 65Gbps.
F.	The switch shall be Vigitron model Vi30406U. 
G.	Standard Ethernet Ports:
2.	The device shall have 4 standard Ethernet ports and 2 SFP ports in a compact housing. The Ethernet port shall comply with: 
a.	IEEE 802.3u 100BaseT 
b.	IEEE 802.3az 1000BaseT 
c.	IEEE 802.3bz 2500BaseT 
d.	IEEE 802.3ae for 10G
2.	The SFP port shall comply with MSA standards
a.	Compatible with:
I.	Multimode
II.	Single mode 
b.	Compatible with: 
I. 100Mbps- UTP
II.1000Mbps network speeds- UTP & Fiber
III.2500Mbps network speeds-UTP & Fiber
IV. 10Gbps network speeds-Fiber 
3.	The standard ports of switch shall support standard Ethernet UTP connection distances up to 100m.
4.	The Fiber port shall be able to operate at 1000/2500Mbps/10Gbps
G.	Port bandwidth settings shall be done automatically.
H.	External Power supply: 48VDC -57VDC up to 400W. 
	a. The switch shall have two DC inputs.
	b. If used, each can serve as backup power supply to each other 
	c. The use of both DC power inputs shall not be required for operation. 
I.	PoE allocation of each port shall accomplished via programming.

J.	The switch shall provide an overall PoE budget, depending upon its power input either by PoE or external power supply. 
1.	When is powered by an external power supply: 
a.	Up to 90W shall be available at each port compliant to: 
III.	802.3af/Class 0-3
IV.	802.3at/Class 4 
V.	802.3bt/Class 5-8
b.	Legacy nonstandard High PoE up to 72W
c.	A DC power input of 380W @ 56 VDC shall be required to have 4 UTP ports provide 802.3bt Class 8 @ 90W  
K.	The switch shall power directly from a DC PoE compliant power source. 
1.	The level of DC PoE compliant power applied shall determine the amount of PoE power available for connected devices.
L.	The switch shall have the following Network programming features using Vigitron’s MPoE™ firmware: 
1.	IP Address
2.	Subnet Mask
3.	Gateway
M.	The switch shall the following log in programming
1.	Assignment and ability to change username
2.	Assignment and ability to change password 
N.	The switch shall the following error message communications
1.	Via Syslog port 514 assignment
2.	Communication via: 
a.	Broadcast
b.	Up to 5 specific IP addresses 
3.	Switch shall provide comprehensive Syslog messaging to include: 
a.	System (switch)given name via operator programming
b.	System location given name via operator programming
c.	IP address of device connected to port
d.	Physical port number
e.	Port status/Port fault
f.	Time and date shall be inserted by the computer receiving the message. 
4.	Syslog messages shall be compatible with any software or switch function capable of receiving syslog messages.
5.	Vigitron shall make available at no charge a copy of SysCap™ for capturing and displaying syslog messages.
O.	The switch shall have the ability to download and save programmed configurations
P.	The switch shall have the ability to upload firmware
Q.	The switch shall provide for a naming convention for: 
1.	The switch 
2.	For individual ports.
R.	The switch shall have the following PoE programming: 
a.	Class defined
b.	User define by inputting and individual power amount
1.	PoE control
a.	Port PoE on
b.	Port PoE off
c.	Force power- shall provide protect PoE power level if connected devices PD’s is not detected. 
S.	PoE Port monitoring: 
1.	Total PoE Budget
2.	Input voltage
3.	Allocated PoE (programmed) 
4.	Remaining PoE power
5.	Individual port Power consumption in Watts
T.	PoE status:
1.	Port PoE as on or off
2.	Class detected. 

U.	The switch shall have the following Autochecking functions for determining device connection and PoE
1.	Enter IP address for the connected PoE Port 
2.	Enable Port for Autochecking 
3.	Disable port for Autochecking 
4.	Detect if entering IP address is valid for the connected device 
5.	Set value in between checks
6.	Set the number of failed attempts prior to stopping autochecking 
7.	Set the number of total attempts. 

V.	The switch shall have the unique ability to confirm setting for: 
1.	PoE 
2.	Autochecking 
3.	On the same GUI screen used for programming and informing the operator: 
a.	Without having to change the GUI screen 
b.	Focus on the specific location and problem

W.	The switch shall be able to pass Jumbo frames up to 9600 bytes 
 
2.04	DATA SPECIFICATIONS
A.	Data Interface: Passage of Data Compliant to -
1.	RFC 768 UDP
2.	RFC 2068 HTTP
3.	RFC 793 TCP
4.	RFC 791 IP
5.	RFC 1783 TFTP
6.	RFC 894 IP over Ethernet
7.	RFC 2544 TCP/IP Packet Transmission
B.	Data Rate: 100/1000Mbps
C.	Data Connections: 
1.	5 Standard Ethernet Ports
2.	1 Fiber port

2.05	SPECIFICATIONS AND FEATURE SETS
A.	The Vi30406U transmits and receives Ethernet data. 
1.	Internal bandwidth shall be constant with no more than a 2% decrease, when the input signal varies from a size of 64 bytes to 10K bytes using bidirectional transmission. 
2.	Internal bandwidth shall be constant over the quoted extended distance with no more than 2% decrease when: 
a.	Bidirectional signals are transmitted with a packet size of 10K bytes.
b.	Unidirectional signals are transmitted with a packet size of 10K bytes.
c.	Bandwidth shall remain the same for both upload and download operation.
B.	Packet losses shall be at 2% or less at packet sizes, ranging from 64 bytes to 10K bytes bidirectional unidirectional up to network port speeds of 10G..
C.	Packets per second (PPS) shall not vary more than 2% at packet sizes, ranging from 64 bytes to 9600 bytes bidirectional transmission. 
D.	Maximum distance from switch port to device shall be 328 ft. (100m) for data and PoE.. 
E.	Each port shall be continuously monitored for potential overcurrent conditions. 
F.	The device must be able to provide PoE compliant to IEEE 802.3af/at/bt standards, Class 0-8 when connected to a PoE powered device.
G.	The switch shall support IEEE 802.1Q.

H.	The Switch shall have two DC input power connections allowing one to serve as back up in the event of a primary power source failure. 
I.	The Vi30406U will have two Watchdogs:
1.		Input power in the form of voltage will be monitored. If voltage falls outside the range of 42VDC to 59VDC power will shut down to protect the midspan and its connected devices.
2.		Internal communications, including the microprocessor, will be monitored every 15 seconds. In the event of stalled or frozen communications the system will issue a 
reset restoring programming and operations 

2.06	CONNECTORS
A.	DC Power Inlet: 2-pin Pluggable terminal block x 2
B.	Standard Ethernet: RJ-45, IEC 60603-7
C.	Fiber Optics: SFP socket MSA Compliant 

2.07	ELECTRICAL SPECIFICATIONS
A.	External Power Supply: 400W @ 54V for all ports provide IEEE 802.3af/at/bt compliant PoE. 
B.	Port PoE Power Outputs (depending on external or PoE power supplied): 
1.	15.4W compliant to IEEE 802.3af ports
2.	36W complaint to IEEE 802.3at Type 1 and Type 2 
3.	90w complaint to IEEE 802.3bt  
4.	72W complaint to most nonstandard high PoE 
C.	Power consumption shall be 12W for standby functions.
2.08	MECHANICAL SPECIFICATIONS (Engineering to supply) 
A.	Dimensions (H x W x L): 1.8x4.8x4.2 in., 4.6x12.2x10.6 cm (HxWxL)
B.	Finish: Device shall be constructed of a metal enclosure. 
C.	Weight: 1.03 lb (470 g)
D.	Mounting: Desktop, Wall mount, DIN Rail

2.09	ENVIRONMENTAL SPECIFICATIONS
A.	Operating Temperature: 40˚C to +70˚C 
B.	Storage Temperature: -40˚C to +85˚C
C.	Relative Humidity: 0% to 95% (non-condensing)
2.10	REGULATORY AGENCIES/APPROVALS AND LISTINGS
A.	FCC Part 15, Subpart A
B.	Emission Standards: 
1.	FCC Part 15, Subpart B, Class A
2.	EN 55022:2006+A1:2007
3.	EN 61000-3-2:2006+A1:2009+A2:2009
4.	EN 61000-3-3:2008
5.	EN 55024:1998+A1:2001+A2:2003
C.	RoHS
D.	CE
2.11	STANDARD ACCESSORIES
A.	Operations Manual

2.12	MANUFACTURED UNITS REFERENCE TABLES
Product	Description	IEEE/Ansi Standards	
Vi30406U	6-port PoE Powered PoE Network Switch 	IEEE 802.3af
IEEE 802.3at
IEEE 802.3bt
IEEE 802.3az
IEEE 802.3bz
IEEE 802.3ac
IEEE 802.1p
IEEE 802.3q	
Table A. Compatible ANSI/ IEEE Standards

Product	Compatible Ethernet Equipment	
Vi30406U 	All products are compliant to standard IP Ethernet protocols.	
Table B. Compatible Ethernet Equipment 

Vigitron reserves the right to change products or specifications without notice.

END OF SECTION