# Vi22116

P1

P2

P3

P4

P5

P6

P7

P8

P9

P10

P11

P12

P13

P14

P15

P16

Autochecking
Port 1:The IPv4 address of the device on port 1 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 2:The IPv4 address of the device on port 2 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 3:The IPv4 address of the device on port 3 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 4:The IPv4 address of the device on port 4 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 5:The IPv4 address of the device on port 5 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 6:The IPv4 address of the device on port 6 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 7:The IPv4 address of the device on port 7 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 8:The IPv4 address of the device on port 8 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 9:The IPv4 address of the device on port 9 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 10:The IPv4 address of the device on port 10 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 11:The IPv4 address of the device on port 11 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 12:The IPv4 address of the device on port 12 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 13:The IPv4 address of the device on port 13 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 14:The IPv4 address of the device on port 14 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 15:The IPv4 address of the device on port 15 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port
Port 16:The IPv4 address of the device on port 16 |  |  | Status: |  | Enable Enable autochecking of device on this port Disable Disable autochecking of device on this port

Autochecking Setting
Duration (80 - 200s): Time between device checks |
Failed Threshold (3 - 7 Times): The number of failed tests before attemtping reboot |
Reboot Attempts (1 - 5 Times): The number of restart attempts before disabling power |